|  |  |  |
| --- | --- | --- |
|  | DocCoverBackground20080320  Mission Name  Core Flight System (CFS)  ***Data Storage (DS)***  ***Version 2.4.0.0***  APPLICATION USER’S GUIDE  Flight Software Systems Branch – Code 582  Version 1.1 – 1/20/15  582-2013-001 | |
| MeatBallSmaller_200dpi | | Goddard Space Flight Center |
| Greenbelt, Maryland |
| National Aeronautics and  Space Administration | | |

Forword

This Core Flight System (CFS) Data Storage (DS) Application User’s Guide provides guidance for the Flight Operations Team (FOT) for the CFS DS Application.

This is one of a set of enhanced User’s Guides for the CFS Product Documentation Suite. While the main audience is the FOT, the Guides also help serve the needs of flight software developers; Flight Software Sustaining Engineering (FSSE), Integration and Test (I&T), and others who support missions which use CFS.

This generic CFS DS Guide is set up so that missions can convert it into a mission-specific guide.



Update History

| Version | Date | Description | Affected Pages |
| --- | --- | --- | --- |
| Draft 0.1 | 04/10/13 | 1st Draft | All |
| 1.0 | 6/24/13 | First Release | All |
| 1.1 | 01/20/15 | Added failed table load information to sections 3.1 and 3.2 | 3-1 |
|  |  |  |  |
|  |  |  |  |

Contents

[Chapter 1. Introduction to the CFS DS User’s Guide 1-1](#_Toc409550314)

[1.1 Purpose and Scope of this Guide 1-1](#_Toc409550315)

[1.2 Acknowledgements 1-1](#_Toc409550316)

[1.3 Conventions and Terminology 1-1](#_Toc409550317)

[1.4 Related Documents 1-2](#_Toc409550318)

[1.5 Assumptions 1-2](#_Toc409550319)

[1.5.1 Personnel 1-2](#_Toc409550320)

[1.5.2 CFS DS Application 1-3](#_Toc409550321)

[1.6 How to Use this Document 1-3](#_Toc409550322)

[1.6.1 Providing Feedback 1-3](#_Toc409550323)

[1.7 Acronyms and Abbreviations 1-4](#_Toc409550324)

[Chapter 2. Introduction to the CFS DS Application 2-1](#_Toc409550325)

[2.1 Heritage 2-1](#_Toc409550326)

[2.2 CFS DS Overview 2-1](#_Toc409550327)

[2.2.1 Writing Table-Defined Data Packets into Files 2-1](#_Toc409550328)

[2.2.2 Inputs to DS 2-1](#_Toc409550329)

[2.2.3 Filtering Data Packets 2-2](#_Toc409550330)

[2.2.3.1 Packet Filter Table 2-2](#_Toc409550331)

[2.2.3.2 Filtering by Sequence 2-3](#_Toc409550332)

[2.2.3.2.1 Filtering by Sequence, Example 1 2-3](#_Toc409550333)

[2.2.3.2.2 Filtering by Sequence, Example 2 2-4](#_Toc409550334)

[2.2.3.3 Filtering by Spacecraft Time 2-4](#_Toc409550335)

[2.2.3.3.1 Filtering by Time, Example 1 2-5](#_Toc409550336)

[2.2.3.3.2 Filtering by Time, Example 2 2-6](#_Toc409550337)

[2.2.3.3.3 Filtering by Time, Example 3 2-7](#_Toc409550338)

[2.2.3.3.4 Filtering by Time, Example 4 2-7](#_Toc409550339)

[2.2.3.3.5 Filtering by Time, Example 5 2-8](#_Toc409550340)

[2.2.3.3.6 Filtering by Time, Example 6 2-9](#_Toc409550341)

[2.2.4 Writing Destination Files 2-9](#_Toc409550342)

[2.2.4.1 More about DS Filenames 2-10](#_Toc409550343)

[2.2.4.2 Primary File Header 2-11](#_Toc409550344)

[2.2.4.3 Secondary File Header 2-11](#_Toc409550345)

[2.2.4.4 Updates by Command vs. Updates by Table 2-12](#_Toc409550346)

[2.2.4.5 Closing Files 2-12](#_Toc409550347)

[2.3 DS Software Context 2-13](#_Toc409550348)

[2.3.1 System Applications 2-14](#_Toc409550349)

[2.3.2 CI Application 2-14](#_Toc409550350)

[2.3.3 cFE SB Application 2-14](#_Toc409550351)

[2.3.4 SCH Application 2-15](#_Toc409550352)

[2.3.5 cFE Table Services (TBL) Application 2-15](#_Toc409550353)

[2.3.6 cFE Time (TIME) 2-15](#_Toc409550354)

[2.3.7 Housekeeping (HK), Stored Command (SC) 2-15](#_Toc409550355)

[Chapter 3. CFS DS Normal Operations 3-1](#_Toc409550356)

[3.1 DS Modes of Operation 3-1](#_Toc409550357)

[3.2 DS Operation 3-1](#_Toc409550358)

[3.2.1 Filtering 3-2](#_Toc409550359)

[3.2.2 Determining What Message IDs Are To Be Stored 3-2](#_Toc409550360)

[3.2.3 Determining Where Files Are Being Stored 3-2](#_Toc409550361)

[3.3 Initializing DS 3-2](#_Toc409550362)

[3.3.1 Power-On Reset 3-3](#_Toc409550363)

[3.3.2 Processor Reset 3-3](#_Toc409550364)

[3.4 Event Messages 3-3](#_Toc409550365)

[3.5 Normal DS Packet Processor Operation 3-3](#_Toc409550366)

[3.6 Packet Filter Table Definition 3-4](#_Toc409550367)

[3.7 Destination File Table Definition 3-5](#_Toc409550368)

[Chapter 4. Understanding DS Operational Constraints 4-1](#_Toc409550369)

[4.1 File Constraints 4-1](#_Toc409550370)

[4.1.1 Maximum File Age 4-1](#_Toc409550371)

[4.1.2 Maximum File Size 4-1](#_Toc409550372)

[Chapter 5. Frequently Asked Questions (FAQs) 5-1](#_Toc409550373)

[5.1 How do I downlink the files saved by DS? 5-1](#_Toc409550374)

[5.2 Are there any issues in limiting data? 5-1](#_Toc409550375)

[5.3 How can I keep files open? 5-1](#_Toc409550376)

[Appendix A CFS DS Reference 1](#_Toc409550377)

[A.1 HK Packet Telemetry 1](#_Toc409550378)

[A.2 File Telemetry 6](#_Toc409550379)

[A.3 Configuration Parameters 9](#_Toc409550380)

[A.4 DS Commands 20](#_Toc409550381)

[A.5 Event Messages 35](#_Toc409550382)

[A.5.1 Event Messages - Critical 35](#_Toc409550383)

[A.5.2 Event Messages - Error 35](#_Toc409550384)

[A.5.3 Event Messages - Information 48](#_Toc409550385)

[A.5.4 Event Messages - Debug 50](#_Toc409550386)

[Appendix B Document Notes 1](#_Toc409550387)

[B.1 Mission-Specific Conventions 1](#_Toc409550388)

[B.2 Tailoring This Document 1](#_Toc409550389)

Table of Figures

[Figure 1 Description of Entry in the Packet Filter Table 2-2](#_Toc359842421)

[Figure 2 Filter Factor Parameters - Filtering by Sequence 2-3](#_Toc359842422)

[Figure 3 Filter Factor Parameters - Filtering by Spacecraft Time 2-5](#_Toc359842423)

[Figure 4 DS Application Software Context 2-14](#_Toc359842424)

[Figure 5 DS Overall Flow Control 2-15](#_Toc359842425)

[Figure 6 DS Flow Control Detail (A) - Ground Command 2-16](#_Toc359842426)

[Figure 7 DS Flow Control Detail (B) - Housekeeping Request 2-17](#_Toc359842427)

[Figure 8 DS Flow Control Detail (C) - Store Data 2-18](#_Toc359842428)

[Figure 9 DS Input Packet Flow (Example) 2-19](#_Toc359842429)

Tables

[Table 1 Related Documents 1-2](#_Toc359589349)

[Table 2 Acronyms and Abbreviations 1-4](#_Toc359589350)

[Table 3 Filtering by Sequence – Example 1 2-3](#_Toc359589351)

[Table 4 Filtering by Sequence – Example 2 2-4](#_Toc359589352)

[Table 5 Filtering by Time – Time Code Format from Packet 2-5](#_Toc359589353)

[Table 6 Filtering by Time – Time Code Filter Format 2-5](#_Toc359589354)

[Table 7 Filtering by Time, Example 1 2-6](#_Toc359589355)

[Table 8 Filtering by Time, Example 2 2-6](#_Toc359589356)

[Table 9 Filtering by Time, Example 3 2-7](#_Toc359589357)

[Table 10 Filtering by Time, Example 4 2-8](#_Toc359589358)

[Table 11 Filtering by Time, Example 5 2-8](#_Toc359589359)

[Table 12 Filtering by Time, Example 6 2-9](#_Toc359589360)

[Table 13 Primary File Header Contents 2-11](#_Toc359589361)

[Table 14 Secondary File Header Contents 2-11](#_Toc359589362)

[Table 15 GPM File Header Contents 2-12](#_Toc359589363)

[Table 16 Packet Filter Table Elements 3-4](#_Toc359589364)

[Table 17 Destination File Table Contents 3-5](#_Toc359589365)

[Table 18 Telemetry Data - Application State A-1](#_Toc359589366)

[Table 19 Telemetry Data - Commands Accepted Counter A-1](#_Toc359589367)

[Table 20 Telemetry Data - Commands Rejected Counter A-1](#_Toc359589368)

[Table 21 Telemetry Data - Destination Table Error Counter A-2](#_Toc359589369)

[Table 22 Telemetry Data – Count of Destination File Table Loads A-2](#_Toc359589370)

[Table 23 Telemetry Data - Count of Packets Discarded While DS Was Disabled A-2](#_Toc359589371)

[Table 24 Telemetry Data – Count of Good Updates to Secondary Header A-2](#_Toc359589372)

[Table 25 Telemetry Data – File Update Error Counter A-3](#_Toc359589373)

[Table 26 Telemetry Data – File Write Counter A-3](#_Toc359589374)

[Table 27 Telemetry Data - Total Number of File Write Errors A-3](#_Toc359589375)

[Table 28 Telemetry Data - Filtered Packet Counter A-3](#_Toc359589376)

[Table 29 Telemetry Data – Packet Filter Table Error Counter A-4](#_Toc359589377)

[Table 30 Telemetry Data – Packet Filter Table Load Counter A-4](#_Toc359589378)

[Table 31 Telemetry Data - Count of Packets Discarded - Packet Has No Filter A-4](#_Toc359589379)

[Table 32 Telemetry Data - Passed Packet Counter A-5](#_Toc359589380)

[Table 33 Telemetry Data - File Enable State A-6](#_Toc359589381)

[Table 34 Telemetry Data - File Age A-6](#_Toc359589382)

[Table 35 Telemetry Data - Filename A-6](#_Toc359589383)

[Table 36 Telemetry Data –File Rate of Growth A-7](#_Toc359589384)

[Table 37 Telemetry Data – File Size A-7](#_Toc359589385)

[Table 38 Telemetry Data – File Open State A-7](#_Toc359589386)

[Table 39 Telemetry Data - Filename Sequence Count A-7](#_Toc359589387)

[Table 40 Configuration Parameter - Application Pipe Depth A-9](#_Toc359589388)

[Table 41 Configuration Parameter - Application Pipe Name A-9](#_Toc359589389)

[Table 42 Configuration Parameter - Destination File Table - Basename Buffer Size A-10](#_Toc359589390)

[Table 43 Configuration Parameter - Destination File Table - Default Table Filename A-10](#_Toc359589391)

[Table 44 Configuration Parameter - Default DS Packet Processor State A-10](#_Toc359589392)

[Table 45 Configuration Parameter - Packet Filter Table - Default Table Filename A-11](#_Toc359589393)

[Table 46 Configuration Parameter - Common Table File - Descriptor Text Buffer Size A-11](#_Toc359589394)

[Table 47 Configuration Parameter - Destination File Table - Number of Files A-11](#_Toc359589395)

[Table 48 Configuration Parameter - Destination File Table - Logical Table Name A-12](#_Toc359589396)

[Table 49 Configuration Parameter - Destination File Table - Extension Buffer Size A-12](#_Toc359589397)

[Table 50 Configuration Parameter - Data Storage File - cFE File Header Description A-13](#_Toc359589398)

[Table 51 Configuration Parameter - Data Storage File - cFE File Header Sub-Type A-13](#_Toc359589399)

[Table 52 Configuration Parameter - File Header Type Selection A-13](#_Toc359589400)

[Table 53 Configuration Parameter - Data Storage File - Minimum Age Limit A-14](#_Toc359589401)

[Table 54 Configuration Parameter - Data Storage File - Minimum Size Limit A-14](#_Toc359589402)

[Table 55 Configuration Parameter - Packet Filter Table - Logical Table Name A-14](#_Toc359589403)

[Table 56 Configuration Parameter - Packet Filter Table - Filters Per Packet A-15](#_Toc359589404)

[Table 57 Configuration Parameter - Make DS Tables Critical A-15](#_Toc359589405)

[Table 58 Configuration Parameter - Filename Sequence Count - Max Counter Value A-15](#_Toc359589406)

[Table 59 Configuration Parameter - Mission Specific Version Number for DS Application A-16](#_Toc359589407)

[Table 60 Configuration Parameter -   
Move Files to Downlink Directory After Close Selection A-16](#_Toc359589408)

[Table 61 Configuration Parameter - Packet Filter Table - Number of Packets A-16](#_Toc359589409)

[Table 62 Configuration Parameter - Destination File Table - Pathname Buffer Size A-17](#_Toc359589410)

[Table 63 Configuration Parameter - Application per Packet Pipe Limit A-17](#_Toc359589411)

[Table 64 Configuration Parameter - Housekeeping Request Frequency A-18](#_Toc359589412)

[Table 65 Configuration Parameter - Filename Sequence Count - Number of Digits A-18](#_Toc359589413)

[Table 66 Configuration Parameter - Data Storage File - Total Filename Size A-18](#_Toc359589414)

[Table 67 Command 0 – No-op A-20](#_Toc359589415)

[Table 68 Command 1 – Reset Housekeeping Telemetry Counters A-20](#_Toc359589416)

[Table 69 Command 2 – Set Enable/Disable State For DS Application A-22](#_Toc359589417)

[Table 70 Command 3 – Set Destination File For Packet Filter Table Entry A-22](#_Toc359589418)

[Table 71 Command 4 – Set Filter Type For Packet Filter Table Entry A-23](#_Toc359589419)

[Table 72 Command 5 – Set Algorithm Parameters For Packet Filter Table Entry A-24](#_Toc359589420)

[Table 73 Command 6 – Set Filename Type For Destination File Table Entry A-25](#_Toc359589421)

[Table 74 Command 7 – Set Enable/Disable State For Destination File Table Entry A-25](#_Toc359589422)

[Table 75 Command 8 – Set Pathname For Destination File Table Entry A-26](#_Toc359589423)

[Table 76 Command 9 – Set Basename For Destination File Table Entry A-27](#_Toc359589424)

[Table 77 Command 10 – Set Extension For Destination File Table Entry A-28](#_Toc359589425)

[Table 78 Command 11 – Set Max File Size For Destination File Table Entry A-29](#_Toc359589426)

[Table 79 Command 12 – Set Max File Age For Destination File Table Entry A-29](#_Toc359589427)

[Table 80 Command 13 – Set Sequence Count For Destination File Table Entry A-30](#_Toc359589428)

[Table 81 Command 14 – Close Destination File A-31](#_Toc359589429)

[Table 82 Command 15 – Get File Info Packet A-32](#_Toc359589430)

[Table 83 Command 16 – Add Message ID to Packet Filter Table A-32](#_Toc359589431)

[Table 84 Command 17 – Close All Destination Files A-33](#_Toc359589432)

[Table 85 Event ID 3 (Critical) - Application Termination A-35](#_Toc359589433)

[Table 86 Event ID 2 (Error) - Application Initialization A-35](#_Toc359589434)

[Table 87 Event ID 6 (Error) - Critical Data Store Access A-36](#_Toc359589435)

[Table 88 Event ID 8 (Error) - Table Create A-36](#_Toc359589436)

[Table 89 Event ID 11 (Error) - Destination File Validation A-37](#_Toc359589437)

[Table 90 Event ID 13 (Error) – Packet Filter Table Validation A-37](#_Toc359589438)

[Table 91 Event ID 14 (Error) - Filename Create A-38](#_Toc359589439)

[Table 92 Event ID 15 (Error) - File Create A-38](#_Toc359589440)

[Table 93 Event ID 16 (Error) - File Write A-39](#_Toc359589441)

[Table 94 Event ID 21 (Error) - Invalid Packet A-39](#_Toc359589442)

[Table 95 Event ID 22 (Error) - Housekeeping Request A-40](#_Toc359589443)

[Table 96 Event ID 32 (Error) - No-op A-40](#_Toc359589444)

[Table 97 Event ID 34 (Error) - Reset Housekeeping Counters A-40](#_Toc359589445)

[Table 98 Event ID 36 (Error) - Set Application Enable/Disable State A-40](#_Toc359589446)

[Table 99 Event ID 38 (Error) - Set Filter File Index A-41](#_Toc359589447)

[Table 100 Event ID 40 (Error) - Set Filter Type A-41](#_Toc359589448)

[Table 101 Event ID 42 (Error) - Set Filter Parameters A-42](#_Toc359589449)

[Table 102 Event ID 44 (Error) - Set Filename Type A-42](#_Toc359589450)

[Table 103 Event ID 46 (Error) - Set File Enable/Disable State A-43](#_Toc359589451)

[Table 104 Event ID 48 (Error) - Set Filename Path A-43](#_Toc359589452)

[Table 105 Event ID 50 (Error) - Set File Basename A-44](#_Toc359589453)

[Table 106 Event ID 52 (Error) - Set Filename Extension A-44](#_Toc359589454)

[Table 107 Event ID 54 (Error) - Set Max File Size A-45](#_Toc359589455)

[Table 108 Event ID 55 (Error) - Set Max File Age A-45](#_Toc359589456)

[Table 109 Event ID 56 (Error) - Set Max File Age A-45](#_Toc359589457)

[Table 110 Event ID 58 (Error) - Set Sequence Count A-46](#_Toc359589458)

[Table 111 Event ID 60 (Error) - Close Destination File A-46](#_Toc359589459)

[Table 112 Event ID 61 (Error) - File Move A-47](#_Toc359589460)

[Table 113 Event ID 63 (Error) - Get File Info A-47](#_Toc359589461)

[Table 114 Event ID 65 (Error) - Add Message ID to Packet Filter Table A-47](#_Toc359589462)

[Table 115 Event ID 67 (Error) - Close All Destination Files A-48](#_Toc359589463)

[Table 116 Event ID 1 (Informational) - Application Initialization Event A-48](#_Toc359589464)

[Table 117 Event ID 10 (Informational) - Destination File Table Validation Results A-49](#_Toc359589465)

[Table 118 Event ID 12 (Informational) – Packet Filter Table Validation Results A-49](#_Toc359589466)

[Table 119 Event ID 31 (Informational) - No-op A-50](#_Toc359589467)

[Table 120 Event ID 7 (Debug) A-50](#_Toc359589468)

[Table 121 Event ID 33 (Debug) A-51](#_Toc359589469)

[Table 122 Event ID 35 (Debug) A-51](#_Toc359589470)

[Table 123 Event ID 37 (Debug) A-51](#_Toc359589471)

[Table 124 Event ID 39 (Debug) A-52](#_Toc359589472)

[Table 125 Event ID 41 (Debug) A-52](#_Toc359589473)

[Table 126 Event ID 43 (Debug) A-53](#_Toc359589474)

[Table 127 Event ID 45 (Debug) A-53](#_Toc359589475)

[Table 128 Event ID 47 (Debug) A-53](#_Toc359589476)

[Table 129 Event ID 49 (Debug) A-54](#_Toc359589477)

[Table 130 Event ID 51 (Debug) A-54](#_Toc359589478)

[Table 131 Event ID 53 (Debug) A-54](#_Toc359589479)

[Table 132 Event ID 57 (Debug) A-55](#_Toc359589480)

[Table 133 Event ID 59 (Debug) A-55](#_Toc359589481)

[Table 134 Event ID 62 (Debug) A-55](#_Toc359589482)

[Table 135 Event ID 64 (Debug) A-56](#_Toc359589483)

[Table 136 Event ID 66 (Debug) A-56](#_Toc359589484)

[Table 137 Internal Document Styles B-2](#_Toc359589485)

# Introduction to the CFS DS User’s Guide

## Purpose and Scope of this Guide

The primary purpose of this Application User’s Guide is to help the Flight Operations Team (FOT) understand the DS application.

Many other purposes will be found for this Guide, including helping mission flight software personnel populate the ground system Record Definition Language (RDL) files in the ground system used later by the FOT, e.g., Advanced Spacecraft Integration & System Test software (ASIST).

Further purposes of this Guide are to help mission developers, system integration test team members, and FSSE to understand the DS application for their own specific needs, such as using the software to perform certain hardware tests.

If you want a more detailed understanding from a developer or FSSE standpoint, review separately the Doxygen-generated html documentation files, or review the source files directly.

As delivered, this is a generic document ready to insert mission defined values to serve the needs of specific missions.

## Acknowledgements

This Application User’s Guide relies heavily on the content of earlier heritage DS publications, presentations, and interviews with flight software engineers. Appendix A is based on information from CFS DS source code and reformatted for this publication. A publication like this is a team effort - thank you to the developers, the management team, and the entire Code 582 review team.

## Conventions and Terminology

* In this document, *Data Storage Application*, *DS application*, and *DS* are used interchangeably, and refer to the CFS version unless specifically referring to heritage code.
* In this document, *flight controller*, *ground controller*, and *FOT* are used interchangeably.
* In this document, the percent sign (%) when followed by a string may indicate variable text. See Appendix A for references to the text that may be substituted in each case.
* *Core Flight Executive* is abbreviated cFE (lower case “c”).
* *Partition* refers to the top level directory of a storage device. A storage device may be formatted so that it contains multiple partitions. Partitions may be fixed sized file systems or simply directory names.
* *File Location* refers to the full path file specification.
* *Pathname* refers to the full path file specification.
* *Basename* refers to the portion of the DS filename that follows the pathname, and precedes the sequence number.
* *Sequence number* refers to a counter, maintained by DS, which is used to uniquely identify a file. For example, filenames that use the size schema are named using the following notation: Basename + File Sequence Counter + Extension (e.g. InstrumentX12345678.xyz).
* *Full path file specification* refers to the Pathname, plus the Basename, plus a Sequence number, and finally, an extension. DS manages the “filename” as the full path file specification.
* *See Appendix B for more.*

## Related Documents

Documents used in the preparation of this Guide are listed in the table below.

Table 1 Related Documents

| Item No. | Document ID | Document Source |
| --- | --- | --- |
| 1 | N/A | Walling, Scott. *Core Flight System Data Storage (DS) Application  Design As Built [Design Presentation].* Greenbelt, MD: Goddard Space Flight Center, Code 582 (Flight Software Branch), 22 Nov 2001. PPT. |
| 2 | N/A | Strege, Susanne. *CFS Data Storage (DS) User's Guide.* Greenbelt: NASA Goddard Space Flight Center, Code 582, CFS Product Development Team, 1 March 2013. Doxygen Output. HTML. |
| 3 | 582-2008-008 | *CFS DS Requirements V1\_1 080111.* Greenbelt: NASA Goddard Space Flight Center, Code 582, Flight Software Systems Branch, 1 August 2011. PDF. |
| 4 | 464-FSW-HDBK-0138 | Steven Slegel. *Solar Dynamics Observatory (SDO) Telemetry Output (TO) Users Guide Version 2.0.* Greenbelt: NASA Goddard Space Flight Center, SDO Flight Software Product Development, 18 April 2007. DOC. |

## Assumptions

### Personnel

This Application User’s Guide assumes the primary reader is a member of the FOT or the equivalent.

### CFS DS Application

The following list summarizes the assumptions made about the CFS DS Application as documented in this Guide:

* The CFS DS code has not been modified.
* The CFS DS Application has been configured using the standard CFS DS configuration parameters.
* The cFE Application Programming Interface (API), and Operating System Abstraction Layer (OSAL) are being used.
* Consultative Committee for Space Data Systems (CCSDS) File Delivery Protocol (CFDP) is being used.
* DS assumes that a file system is being used. In order to get the data to the ground, a file transfer mechanism such as CFDP must be used; DS is not responsible for transferring the data.
* DS does not provide the interface to the hardware used for storing the data. DS simply writes to files and assumes that the interfaces required to write to the devices/partitions are available.
* Use of Electrically Erasable Programmable Read Only Memory (EEPROM) generally requires that writing be enabled prior to writing. DS does not provide this capability.
* A command is sent to DS to request DS housekeeping messages (i.e. from the CFS Scheduling [SCH] application).
* Until a disk is created and partitions formatted for DS to use to store the destination file, the DS application should be disabled. Once the disk has been created, and partitions formatted, the Enable command can be sent to enable the DS application to start opening and writing to files, as defined in the Destination File Table.
* The command mnemonics shown in this Guide were developed for, and assume the use of, ASIST ground control software.

## How to Use this Document

Use this Application User’s Guide as a learning tool before launch. Use the Appendix as a reference tool after launch. Read it offline as a paper printout, or search the electronic file. Use the Guide along with Doxygen generated .html files for more complete understanding. In contrast to this Guide, the Doxygen generated html files are primarily targeted to developers and FSSE.

Experienced flight controllers may only need to browse the Guide, and use the Appendix as needed. New flight controllers may wish to get more familiar with the entire Guide well before needing to rehearse operational scenarios or set up flight software procedures (“procs”).

### Providing Feedback

For CM reasons, if you find any item in this Guide that is in error, or want to be informed of any updates, please email feedback to the cFE/CFS PDL for validation and routing. As of the date of publication, the cFE/CFS PDL is Susie Strege (susanne.L.strege@nasa.gov).

Besides corrections of any errors, the CFS team is interested in your ideas on improvements that help understanding.

## Acronyms and Abbreviations

Acronyms and abbreviations in this publication are shown in Table 2 below. Telemetry, command mnemonics, and similar terms are not shown here.

Table 2 Acronyms and Abbreviations

| Abbreviation or Acronym | Description |
| --- | --- |
| ACS | Attitude Control System |
| API | Application Programming Interface |
| ApID | Application ID, also known as Message ID |
| ASIST | Advanced Spacecraft Integration & System Test software |
| C&DH | Command and Data Handling |
| CCSDS | Consultative Committee for Space Data Systems |
| CC | Command Code |
| CDS | Critical Data Store |
| CFDP | CCSDS File Delivery Protocol |
| cFE/CFE | Core Flight Executive |
| CFS | Core Flight System |
| CI | Command Ingest |
| Cmd | Command |
| DS | CFS Data Storage application |
| EEPROM | Electrically Erasable Programmable Read Only Memory |
| FOT | Flight Operations Team |
| FSSE | Flight Software Sustaining Engineering |
| GN&C | Guidance Navigation and Control |
| GPM | Global Precipitation Measurement |
| GSFC | Goddard Space Flight Center |
| HK | Housekeeping Application |
| I&T | Integration and Test |
| ITOS | Integration Test and Operations System |
| LRO | Lunar Reconnaissance Orbiter |
| LSB | Least Significant Bit |
| MID | Message ID |
| MSB | Most Significant Bit |
| No-op | No operation |
| OS | Operating System |
| OSAL | Operating System Abstraction Layer |
| PDL | Product Development Lead |
| RAM | Random-Access Memory |
| RDL | Record Definition Language |
| SB | cFE Software Bus Application |
| SC | Stored Command application |
| SCH | CFS Scheduling Application |
| SDO | Solar Dynamics Observatory |
| ST-5 | Space Technology 5 |
| TBL | cFE Table Services Application |
| TIME | cFE Time Application |
| TLM | Telemetry |
| TO | Telemetry output |
| VCDU | Virtual Channel Data Unit |

This page intentionally blank.

# Introduction to the CFS DS Application

This chapter addresses the theory and internal operation of the CFS DS application.

## Heritage

The CFS DS code derives from the Lunar Reconnaissance Orbiter (LRO) mission, which used data storage files. Most other heritage missions, such as the Solar Dynamics Observatory (SDO) and Space Technology 5 (ST-5), stored the data as messages or Virtual Channel Data Units (VCDUs) in buffers. In the CFS DS design, data is stored as cFE Software Bus messages in files, rather than buffers.

The CFS team took LRO’s DS application and made it CFS compliant, adding configuration parameters in place of hard coded parameters, and making other changes to fit it into the larger CFS architecture.

## CFS DS Overview

The CFS DS application performs three basic functions:

* It writes table-defined data packets (cFE Software Bus messages), into files for later transmission to the ground.
* It performs filtering on received packets, prior to storage.
* It stores files on a file system.

DS references two tables, the Packet Filter Table and the Destination File Table.

### Writing Table-Defined Data Packets into Files

DS writes cFE Software Bus messages to table-defined data storage files. These files are generally stored on a device such as a solid state recorder. However, they could be stored on any storage device with a file system.

DS has no file download or playback capabilities; another application such as CFDP must be used to transfer to the ground the files created by DS.

### Inputs to DS

Any cFE Software Bus message (a CCSDS compliant packet) can be written to files by DS.

* The cFE Software Bus (SB) application routes cFE Software Bus messages to DS. The messages can come from a number of sources; these sources can include ground commands via a command ingest application.
* The cFE Table Services application provides DS with knowledge of updates to the DS Destination File Table and the DS Packet Filter Table.

DS keeps a list of Message IDs (also known as Application ID, or *ApID* entries) to which it has subscribed. For fast look up of packet ApIDs, DS creates a hash table.

For the Packet Filter Table (though not the Destination File Table) when DS receives notice from cFE Table Services that a new table commit is pending, DS unsubscribes to the ApID entries in the old Packet Filter Table before the new table data is copied into DS table space. Typically the table service command sequence is load/validate/commit. DS then subscribes to the new ApIDs and creates a new hash table.

### Filtering Data Packets

DS can store cFE Software Bus messages at different rates using two possible filtering schemes (Sequence or Time Based filtering) allowing "N of X" messages to be stored starting at offset 0 (zero).

#### Packet Filter Table

Each Packet Filter Table is identified by a character string descriptor whose length is configurable by the mission. Typically, a mission may set up multiple versions of the Packet Filter Table, such as for I&T; launch; orbit insertion; Guidance and Navigation; Attitude Control System (ACS); and nominal, for example.

The Packet Filter Table contains a *list of packets* (Message IDs) that DS will process, along with *filtering information* specific to each packet.

For each Message ID, the Packet Filter Table specifies the *storage and* *filtering information* shown in Figure 1 below.

|  |
| --- |
| **Storage Element**   * A zero based index into the Destination File Table   **Filtering Elements**   * The type of filter used by this entry: by count or by time (the filter type defines whether the input data is a value derived from the packet timestamp, or if the input data is derived from the header sequence count) * The N and X arguments passed into the Filter algorithm that allows “N of every X” data packets to be stored * The O argument passed into the Filter algorithm Filter that allows data packets to be stored starting with the packet at offset “O” |

Figure Description of Entry in the Packet Filter Table

The configuration parameter DS\_FILTERS\_PER\_PACKET specifies the **storage and filtering information** per packet. This allows a packet to be stored in multiple destinations at different rates.

For example, each full entry would contain a Message ID, accompanied by:

[(Storage Element, Filtering Elements)1 , (Storage Element, Filtering Elements)2 , … (Storage Element, Filtering Elements)A ] where A is the number specified by the configuration parameter.

The **filtering elements** includethree (3) 16-bit parameters (N, X, and O). The filter algorithm allows “N of X” cFE Software Bus messages to be stored starting at offset O.

#### Filtering by Sequence

Filtering by sequence uses the packet sequence number to determine if the cFE Software Bus message should be filtered or not.

The filter factor has three parameters and can be expressed in terms of N number of packets out of X number of packets. The offset Y determines the starting point within X for selecting packets.

If X is greater than zero, the message will be stored if and only if the sequence number modulo X is less than N. For example, N=4, X=6 and O=2 will store 4 of 6 messages starting at offset 2.



Figure Filter Factor Parameters - Filtering by Sequence

If the packet sequence number minus Y mod X is less than N then the packet will be output:

**if (((packet\_sequence\_counter - Y) MOD (X)) < N) then**

**output the packet**

**else**

**drop the packet**

**end if**

##### Filtering by Sequence, Example 1

In Filtering by Sequence - Example 1, we send two out of every four packets, offset packet zero. This will send two packets and then skip two packets. If instead one wanted every other packet then one would specify one out of two packets.

Table Filtering by Sequence – Example 1

|  |  |
| --- | --- |
| N | 2 |
| Y | 0 |
| X | 4 |

| **Sequence Number** | **Send** |
| --- | --- |
| 0 | ✓ |
| 1 | ✓ |
| 2 |  |
| 3 |  |
| 4 | ✓ |
| 5 | ✓ |
| 6 |  |
| 7 |  |
| 8 | ✓ |
| 9 | ✓ |
| 10 |  |

##### Filtering by Sequence, Example 2

In Filtering by Sequence - Example 2 we send two out of every four packets, offset packet one. This will send two packets and then skip two packets, starting with packet one:

Table Filtering by Sequence – Example 2

|  |  |
| --- | --- |
| N | 2 |
| Y | 1 |
| X | 4 |

| **Sequence Number** | **Send** |
| --- | --- |
| 0 |  |
| 1 | ✓ |
| 2 | ✓ |
| 3 |  |
| 4 |  |
| 5 | ✓ |
| 6 | ✓ |
| 7 |  |
| 8 |  |
| 9 | ✓ |
| 10 | ✓ |

#### Filtering by Spacecraft Time

Time based filtering uses the Spacecraft time code found in the CCSDS packet secondary header. The filter factor has three parameters and can be expressed in terms of N number of packets out of X number of Seconds/Sub Seconds. Note there are 16 Sub Seconds per Second.

The offset Y determines the starting point within the X for selecting packets. Messages are stored if and only if the message time stamp modulo X is less than N.

Fifteen bits out of the 64-bit CCSDS time code field are used. The constructed 15-bit time stamp used for DS filtering consists of the 11 least significant bits (LSBs) of the seconds field and the four most significant bits (MSBs) of the sub-seconds field. Messages will be stored if and only if the constructed 15-bit time stamp modulo X is less than N.

This type of filtering is rare in that the N value must be set to the desired 15-bit time stamp, which is hard to specify.



Figure Filter Factor Parameters - Filtering by Spacecraft Time

The time code filter factor consists of the least significant 11 bits of the Lo\_Word Seconds (a), and the most significant four bits of the Hi\_Word Sub Seconds (b). Bit 16 is not used (c). For more, see tables below.

Table Filtering by Time – Time Code Format from Packet

|  |  |  |  |
| --- | --- | --- | --- |
| Hi\_Word Seconds | Lo\_Word Seconds | Hi\_Word Sub Seconds | Lo\_Word Sub Seconds |
|  | Xxxxx**aaaaaaaaaaa** | **bbbb**xxxxxxxxxxxx |  |

Table Filtering by Time – Time Code Filter Format

|  |  |  |
| --- | --- | --- |
| c | aaaaaaaaaaa | Bbbb |

The sign of X determines the type of filtering that will be performed:

**if (X = 0) then**

**don't output any packets**

**else if (X > 0) then**

**sequence number filtering**

**else if (X < 0) then**

**time based filtering**

**end if**

If the packet time code (in time code filter format) minus Y mod X (the absolute value in time code filter format) is less than N then the packet will be output.

**if (((packet\_time\_code - Y) MOD (ABS(X))) < N) then**

**output the packet**

**else**

**drop the packet**

**end if**

##### Filtering by Time, Example 1

In Filtering by Time - Example 1, if a packet is generated four times a second, we send one packet per second. An offset of zero (0) will send the first packet generated per second. This works well for synchronous data that is generated at exactly the same time each second.

Table Filtering by Time, Example 1

|  |  |
| --- | --- |
| N | 1 |
| Y | 0 |
| X | 16 |

| **Time ( Sub Seconds)** | **Pkt Gen** | **Send** |
| --- | --- | --- |
| 0 | Pkt | ✓ |
| 1 |  |  |
| 2 |  |  |
| 3 |  |  |
| 4 | Pkt |  |
| 5 |  |  |
| 6 |  |  |
| 7 |  |  |
| 8 | Pkt |  |
| 9 |  |  |
| 10 |  |  |
| 11 |  |  |
| 12 | Pkt |  |
| 13 |  |  |
| 14 |  |  |
| 15 |  |  |
| 16 | Pkt | ✓ |

##### Filtering by Time, Example 2

In Filtering by Time - Example 2, no packets would be sent because no packets are generated in time slot zero (0). Note that the offset must be used to synchronize the time slot that we want to send with the time slot in which the packet is generated. The offset must be set to one (1) to make the filtering work the same as in the previous example.

Table Filtering by Time, Example 2

|  |  |
| --- | --- |
| N | 1 |
| Y | 0 |
| X | 16 |

| **Time ( Sub Seconds)** | **Pkt Gen** | **Send** |
| --- | --- | --- |
| 0 |  |  |
| 1 | Pkt |  |
| 2 |  |  |
| 3 |  |  |
| 4 |  |  |
| 5 | Pkt |  |
| 6 |  |  |
| 7 |  |  |
| 8 |  |  |
| 9 | Pkt |  |
| 10 |  |  |
| 11 |  |  |
| 12 |  |  |
| 13 | Pkt |  |
| 14 |  |  |
| 15 |  |  |
| 16 |  |  |
| 17 | Pkt |  |

##### Filtering by Time, Example 3

In Filtering by Time - Example 3, if a packet is generated four times a second, we send one packet per second. An offset of four (4) will send the second packet generated per second. This works well for synchronous data that is generated at exactly the same time each second. Note that an offset of one, two, or three (1, 2, or 3) will not send any packets because packets are not generated in those time slots.

Table Filtering by Time, Example 3

|  |  |
| --- | --- |
| N | 1 |
| Y | 4 |
| X | 16 |

| **Time ( Sub Seconds)** | **Pkt Gen** | **Send** |
| --- | --- | --- |
| 0 | Pkt |  |
| 1 |  |  |
| 2 |  |  |
| 3 |  |  |
| 4 | Pkt | X |
| 5 |  |  |
| 6 |  |  |
| 7 |  |  |
| 8 | Pkt |  |
| 9 |  |  |
| 10 |  |  |
| 11 |  |  |
| 12 | Pkt |  |
| 13 |  |  |
| 14 |  |  |
| 15 |  |  |

##### Filtering by Time, Example 4

In Filtering by Time - Example 4, if a packet is generated 10 times a second, we send two packets per second. Note that the X is 1/2 a second or eight sub seconds.

Table Filtering by Time, Example 4

|  |  |
| --- | --- |
| N | 1 |
| Y | 0 |
| X | 8 |

| **Time ( Sub Seconds)** | **Pkt Gen** | **Send** |
| --- | --- | --- |
| 0 | Pkt | X |
| 1 |  |  |
| 2 | Pkt |  |
| 3 |  |  |
| 4 | Pkt |  |
| 5 | Pkt |  |
| 6 |  |  |
| 7 | Pkt |  |
| 8 | Pkt | X |
| 9 |  |  |
| 10 | Pkt |  |
| 11 |  |  |
| 12 | Pkt |  |
| 13 | Pkt |  |
| 14 |  |  |
| 15 | Pkt |  |

##### Filtering by Time, Example 5

In Filtering by Time - Example 5, if a packet is generated four times a second, we send two packets per second. Note that in this example packets are not generated at exactly the same times each second and we will not see every packet we expect.

Table Filtering by Time, Example 5

|  |  |
| --- | --- |
| N | 1 |
| Y | 0 |
| X | 8 |

|  |  |  |
| --- | --- | --- |
| **Time ( Sub Seconds)** | **Pkt Gen** | **Send** |
| 0 |  |  |
| 1 | Pkt |  |
| 2 |  |  |
| 3 |  |  |
| 4 | Pkt |  |
| 5 |  |  |
| 6 |  |  |
| 7 |  |  |
| 8 | Pkt | X |
| 9 |  |  |
| 10 |  |  |
| 11 |  |  |
| 12 |  |  |
| 13 | Pkt |  |
| 14 |  |  |
| 15 |  |  |

##### Filtering by Time, Example 6

To fix the problem in example 5, and to get every other packet, set the N to 3. This will send the packet as long as it falls within 3 slots (3 packets every 8 sub seconds).

Table Filtering by Time, Example 6

|  |  |
| --- | --- |
| N | 3 |
| Y | 0 |
| X | 8 |

| **Time ( Sub Seconds)** | **Pkt Gen** | **Send** |
| --- | --- | --- |
| 0 |  |  |
| 1 | Pkt | X |
| 2 |  | X |
| 3 |  |  |
| 4 | Pkt |  |
| 5 |  |  |
| 6 |  |  |
| 7 |  |  |
| 8 | Pkt | X |
| 9 |  |  |
| 10 |  |  |
| 11 |  |  |
| 12 |  |  |
| 13 | Pkt |  |
| 14 |  |  |
| 15 |  |  |

### Writing Destination Files

The Destination File Table defines a list of data storage files along with creation information specific to each file. A configuration parameter determines the maximum number of files that can be defined in the Destination File Table.

The Destination File Table defines data storage files as shown below:

*Filename*

* The file path
* The base portion of the filename
* The filename extension (including the dot)
* The file type: by count or by time (the file type denotes whether the file name includes an incrementing value or the Spacecraft time)

*State*

* The enable/disable state for this destination file

*Limits*

* The file **size** at which to close the file and open a new one
* The file **age** at which to close the file and open a new one

*Sequence*

* An initial value for a numerical sequence to be appended to the filename before the extension

As each file is closed, if the file type is by count, then the file type counter is incremented for the next file to be opened. (If the file type is by time, then the current Spacecraft time is always used, and Spacecraft time is always changing, resulting in a unique filename for each file.)

Each DS filename contains characters derived from a filename sequence counter or from the current Spacecraft time at the time the file was created.

Files are generally organized in a way that is meaningful to each mission. For example, some missions may wish to include all housekeeping data into one set of files, while others may wish to split out certain types of housekeeping data into separate files. The Destination File Table contains the scheme, or definitions, for the files into which cFE Software Bus messages will be saved.

Any packet sent on the Software Bus can be stored in a file. Typically Command and Data Handling (C&DH) housekeeping telemetry is saved into one file, for example, and Guidance, Navigation and Control (GN&C) housekeeping in another file. Instrument data may be saved in yet another file.

Science data, if it is low volume, may also be saved, though typically science data is larger volume and handled by a separate, dedicated module.

The Destination File Table is typically set up before launch and is not frequently changed.

#### More about DS Filenames

DS manages the filename as the Pathname, plus the Basename, plus a Sequence number, and finally, an extension. The entire length of the filename must not exceed the length specified by the OSAL configuration parameter OS\_MAX\_PATH\_LEN.

Each entry in the Destination File Table contains a character string definition for Pathname, Basename and Extension and a type selection for the Sequence portion of the filename.

Depending on the Filename Type, DS will construct a character string that represents either the value of a filename sequence counter specific to that particular Destination File Table entry, or the current time of day in the format YYYYDDDHHMMSS.

If the file is sequence-based, the sequence characters will be based upon the next sequence number. For example, if the initial value for a numerical sequence = 1, Pathname = /ram and Basename = seq and extension = .dat, then the file would be named /ram/seq00000100.dat for the 100th file.

* For the maximum value a file sequence count will reach before rollover to zero, refer to the mission-specific DS config. parameter DS\_MAX\_SEQUENCE\_COUNT.
* For the number of filename sequence count digits used when the filename type has been set to "count" rather than "time," refer to the mission-specific DS configuration parameter DS\_SEQUENCE\_DIGITS.

***Tip:*** *As a reminder, the only portion of* ***sequence-based*** *filenames that change is the sequence counter, as assigned to the file at the time the file is opened. The path, base, and extension are constant as defined in the Destination File Table, unless changed by command and/or a table load.*

***Tip:*** *Note that in sequence-based filenames the sequence count always rolls over to zero. The rollover to zero is not configurable to a different number. In practice, missions often reset the sequence count each orbit, or whenever the mission changes the base part of the filenames to identify a new data set. So the result is that in practice the numbers seldom get large enough to roll over.*

If the file is **time-based**, the characters will be in the form YYYYDDDHHMMSS. For example if the file was created on day 123 at 14:15:22 using Pathname = /ram, Basename = tim and extension = .dat, the file would be named /ram/tim2010123141522.dat.

***Tip:*** *As a reminder, the only portion of* ***time-based*** *filenames that change is the Spacecraft time, as assigned to the file at the time the file is opened. The path, base, and extension are constant as defined in the Destination File Table, unless changed by command and/or a table load.*

For the path, base and extension, refer to the mission-specific File Table for the appropriate entry.

#### Primary File Header

Each DS destination file contains a primary cFE file header with the information shown below.

Table Primary File Header Contents

| Element | Description |
| --- | --- |
| Content Type | Specifies cFE compliant files. Value will be set to 0x63464531 |
| SubType | Specifies type of file. Value is defined via DS configuration parameter |
| Primary header length | Length of primary header |
| Spacecraft ID | Spacecraft that generated the file |
| Processor ID | Processor that generated the file |
| Application ID | Application that generated the file |
| File creation time | In seconds |
| File creation time | In sub-seconds |

#### Secondary File Header

Each DS destination file contains a mission-optional secondary file header. Each mission has the option (controlled by configuration parameter) to choose not to include a secondary file header.

The format of the secondary file header is also configurable. This version of the DS application includes the ability to generate the CFS DS standard file header or the file header that conforms to the specifications of the Global Precipitation Measurement (GPM) mission. The tables below shows the contents of the DS standard file header and GPM file header.

Table Secondary File Header Contents

| Element | Description |
| --- | --- |
| File close time | Seconds portion of Spacecraft time that the file was closed |
| File close time | Subseconds portion of Spacecraft time that the file was closed |
| File table index | Destination File Table index |
| File name type | File type (count vs. time) |
| Qualified filename | Full path specification of file |

Table GPM File Header Contents

| Element | Description |
| --- | --- |
| Source ID | String of four characters identifying the source of the file data |
| Sequence ID | File generation counter |
| File start time | Seconds portion of Spacecraft time that the file was opened |
| File stop time | Seconds portion of Spacecraft time that the file was closed |
| File size | Total size of the file in bytes |
| Spare | Spare bytes (20 total) |

#### Updates by Command vs. Updates by Table

For configuration management, some missions prefer to make changes only by changing tables via a table load where a new table file can be uplinked via CFDP and loaded via cFE Table Services. However, DS supports changing individual table entry settings by command. For details, see Appendix A, section A.4, DS Commands.

#### Closing Files

Files can be defined to close at a maximum size (measured in bytes) and a maximum age (measured in seconds). When closed, a new file will be opened.

If the desired **maximum file size** would be exceeded, the application will close the file and open a new one with a unique name according to the rules set up in the Destination File Table. If the desired **maximum age** would be exceeded, the application will close the file and open a new one with a unique name according to the rules set up in the Destination File Table.

However, files are not closed based on whether the filename is sequence based or time based. **Both the file size and file age are checked.** If a file is time based but the file size is exceeded before the time is met, the file will still be closed.

If one wants the file to close by *age* then the file size limit needs to be set unreasonably large. The unreasonably large file size limit should never pass, making age the only meaningful check.

Similarly, if one wants the file to close by *file size* then the age limit needs to be set unreasonably large. The unreasonably large age limit should never pass, making the file size the only meaningful check.

To avoid creating empty files, the desired file size is only verified after the first packet is saved. So the first packet written may cause the file to exceed the desired size.

DS will always have at least one packet in every file. Its size is defined in the Destination File table, and can be changed by the FOT.

cFE Software Bus messages are stored in a file or files in their entirety, i.e. messages are not segmented between files.

## DS Software Context

The figure below shows the software context for the CFS DS Application.



Figure 4 DS Application Software Context

### System Applications

As shown in Figure 4 above, CFS system applications as configured for a particular mission may communicate with DS via message packets via the cFE Software Bus application.

### CI Application

Ground commands are routed through a CI Application, as shown in Figure 4 above.

### cFE SB Application

Message packets which will be filtered and saved by DS arrive via the cFE SB Application. As shown in Figure 4 above, CFS applications communicate with DS via SB.

### SCH Application

The SCH application wakes up DS when SCH requests DS housekeeping data, as shown in Figure 4 above. Additionally, DS subscribes to message packets, and is awakened when it receives those packets.

### cFE Table Services (TBL) Application

As shown in Figure 4 above, DS learns of any updates to the DS Packet Filter Table and Destination File Table through the cFE Table Services (TBL) application.

### cFE Time (TIME)

cFE TIME (the cFE Time application) distributes Spacecraft time of day data used by DS, as shown in Figure 4 above.

### Housekeeping (HK), Stored Command (SC)

As shown in Figure 4 above, any cFE Software Bus messages generated by DS are routed to whatever mission-specific applications subscribe to them, such as the Housekeeping (HK) application, a telemetry output (TO) application, and/or Stored Command (SC) Applications.

Figure 5 below shows the overall program flow of the DS, from start to exit.



Figure 5 DS Overall Flow Control

Figure 6 below shows the flow control of DS for *ground* commands.



Figure 6 DS Flow Control Detail (A) - Ground Command

Figure 7 below shows the flow control of DS for *housekeeping* requests.



Figure 7 DS Flow Control Detail (B) - Housekeeping Request

Figure 8 below shows the flow control of DS for *Store Data*.



Figure 8 DS Flow Control Detail (C) - Store Data

Figure 9 below shows a visual description of how the two DS tables are used to control data storage*.*



Figure DS Input Packet Flow (Example)

This page intentionally blank.

# CFS DS Normal Operations

This chapter addresses the most common issues expected to arise during normal operations.

## DS Modes of Operation

DS can be configured to start up enabled or disabled. A configuration parameter (DS\_DEF\_ENABLE\_STATE) defines the state in which DS will start.

In **enabled mode**, DS will begin to process packets immediately on startup. Processing packets means DS is checking to see if the received CFS Software Bus Message is included in the Packet Filter Table. If the message is included in the Packet Filter Table, DS runs the filtering algorithm to determine if the packet should be written to a file or not.

Upon startup or table update, if the Destination File Table and/or Packet Filter Table have failed to load, DS will not store any messages until both tables are loaded with valid data. Loading the Tables with valid data can be accomplished by using the cFE Table Services commands after creating a Table load image file and uploading it to the spacecraft's file system. Until both tables are loaded with valid data, DS will increment the IgnoredPktCounter for each received packet that is discarded.

The flow of this process is shown starting in Figure 8, DS Flow Control Detail (C) - Store Data, and described below starting in Section 3.2, DS Operation.

In **disabled mode**, DS will ignore message packets contained in the Packet Filter Table that DS has subscribed to until receipt of a valid command to enable the DS Application. DS will not increment the IgnoredPktCounter for each received packet that is discarded when in **disabled mode**.

## DS Operation

When DS is enabled for storage and DS tables have loaded successfully, DS works as follows:

1. When DS receives a cFE Software Bus message that passes the filtering algorithm, the message is stored in a file or files based upon the Packet Filter Table information for that Message ID. The Packet Filter Table points to the index or indexes of the file or files defined in the Destination File Table. Once a message is stored, the DS housekeeping packet provides information about the open file.
2. Each housekeeping cycle, DS evaluates open files to determine if their maximum age has been exceeded. If their maximum age has been exceeded, then DS closes the file. The age test is done at housekeeping time because an old file needs to be closed even if there are no packets being received. Effectively, this means the age is tested about every five seconds or so.
3. The check for maximum size is done as DS receives cFE Software Bus messages. If DS and the destination file are enabled, the destination file is open, and the cFE Software Bus message passes any filtering, then the size check is performed. If the total of the destination file’s current size plus the new cFE Software Bus message size exceeds the file size limit, then the file is closed. DS opens a new file, and writes the cFE Software Bus message to the new file. A minimum of one message is stored in each file.

### Filtering

The Packet Filter Table determines what cFE Software Bus messages DS will store via the Software Bus Message IDs and the rate the incoming messages will be stored. The DS application supports two types of filtering: *sequence number based* filtering and *time based* filtering.

Each filtering type relies on three filter factors, N, X, and O where N of X messages will be stored starting at offset O.

DS may store a single cFE Software Bus message using different filter schemes.

*For more detail on filtering refer to Chapter 2.*

### Determining What Message IDs Are To Be Stored

The Message IDs to be stored are specified in the Packet Filter Table. The currently loaded Packet Filter Table may be dumped via cFE Table Services to obtain a listing of the stored Message IDs. Once the table is dumped and downlinked, the table contents are typically displayed on the mission-specific Packet Filter Table display page in ASIST, Integration Test and Operations System (ITOS), or other ground flight software.

### Determining Where Files Are Being Stored

The locations of the files are determined by both the Packet Filter Table and the Destination File Table. The Packet Filter Table, for each Message ID, indicates the index(s) into the Destination File Table, specifying the file(s) in which the message is to be stored. For details about information in the Packet Filter Table, see Section 2.2.3.1, Packet Filter Table.

The Destination File Table defines data storage files and their location. For details about how the Destination File Table defines data storage files, see Section 2.2.4, Writing Destination Files.

To trace the Message ID to the File entry, both tables must be dumped and downlinked. Once the tables are dumped and downlinked, the table contents are typically displayed on the mission-specific Packet Filter Table display page in ASIST, ITOS, or other ground flight software.

## Initializing DS

During initialization, DS subscribes to cFE Software Bus messages from other applications as defined in the Packet Filter Table.

DS attempts to load the Destination File Table and Packet Filter Table defined in the configuration parameters DS\_DEF\_DEST\_FILENAME and DS\_DEF\_FILTER\_FILENAME upon startup.

If the load fails for either of these tables, DS will still start. However, DS will not store any messages until both tables are loaded with valid data. This can be accomplished by using cFE Table Services commands after creating a table load image file and uploading it to the spacecraft's file system.

### Power-On Reset

On power-on reset, DS performs a cFE application-specific initialization:

1. Initializes housekeeping data and global variables.
2. Registers for cFE Services.
3. Creates Software Bus input pipe.
4. Subscribes to ground commands and housekeeping requests.
5. Creates Packet Filter Table and Destination File Table.
6. Loads table data from default table files.
7. Subscribes to message packets named in the Packet Filter Table.

### Processor Reset

On processor reset, all files that were open before processor reset will be closed, regardless of file size or age.

On processor reset, DS performs the same initialization as power-on reset unless the mission has implemented Critical Data Store (CDS), as described below.

1. If the configuration parameter DS\_MAKE\_TABLES\_CRITICAL is set to “1”, then cFE Table Services will load data for both DS tables from the CDS instead of from the default table data files.
2. Regardless of table criticality, DS will at startup attempt to retrieve the current filename sequence counters and destination enable/disable state values for each entry in the Destination File Table that is also stored in the CDS.

## Event Messages

There are four levels of event types:

* Critical
* Error
* Information
* Debug

The levels are not used for programmatic control by CFS or DS. In other words, CFS and DS do not treat the level labels differently. However, ASIST, ITOS, or other ground flight control software may display event messages in different colors or otherwise differentiate them.

**Debug** level messages are typically used before launch for testing but then reconfigured off to avoid cluttering flight operator telemetry.

## Normal DS Packet Processor Operation

DS files are not created until a packet has passed the filter tests and is ready to be written to the file. This avoids potentially empty files.

Each packet received by DS (including DS commands and the DS housekeeping packet) is processed as a candidate for being written to a file.

If DS is enabled for packet processing, and the Message ID is found in the Packet Filter Table, then the packet filters are processed by evaluating the filter algorithm using parameters specific to each packet filter.

* If any passed packet filter references an enabled entry in the Destination File Table then the packet will be written to that file. A single packet may thus be written to multiple DS files.
* If the DS file does not yet exist, it will be created and initialized with both a cFE file header and a DS secondary file header.

## Packet Filter Table Definition

The Packet Filter Table consists of a series of packet entries. Each packet entry contains the Message IDs for DS to store.

The maximum number of entries is defined by the configuration parameter DS\_PACKETS\_IN\_FILTER\_TABLE.

The number of filters per packet entry, and thus, (1) the maximum number of destination files to which a single packet can be written at a time; and (2) the rate that a single packet can be written to those destination files, is defined by the configuration parameter DS\_FILTERS\_PER\_PACKET.

Table Packet Filter Table Elements

|  |  |
| --- | --- |
| Element | Description |
| File Table Index | The zero based index into the Destination File Table. (Defines which data storage file is associated with this packet filter. It is common for multiple packet filters to reference the same data storage file.) |
| Filter Type | The type of filter used by this entry DS\_BY\_COUNT or DS\_BY\_TIME. (Defines the filter algorithm input data. If Filter Type is time then the input data is a 15 bit value derived from the packet timestamp. If Filter Type is count then the input data is the 14 bit packet header sequence count.) |
| Algorithm\_N | The N argument passed into the Filter algorithm. (The filter algorithm allows “N of every X” data packets to be stored, starting with the packet at offset “O of X”.) |
| Algorithm\_X | The X argument passed into the Filter algorithm. (The filter algorithm allows “N of every X” data packets to be stored, starting with the packet at offset “O of X”.) |
| Algorithm\_O | The O argument passed into the Filter algorithm |

## Destination File Table Definition

The Destination File Table contains the entries described below.

Table Destination File Table Contents

| Element | Description |
| --- | --- |
| Pathname | The full path file specification. Also known as file location. |
| Basename | Contains the base portion of the filename. |
| Extension | Contains the extension (including the dot). |
| Filename Type | Defines the sequence portion of the filename as either an incrementing value (“count”) or time of day. |
| File State | Defines the enable/disable state for this destination file. |
| Max File Size | Close current file when it gets this big. |
| Max File Age | Close current file when it gets this old. |
| Sequence Counter | Initial value for filename sequence counter. This value is referenced only when filename type is “count”. |

This page intentionally blank.

# Understanding DS Operational Constraints

## File Constraints

### Maximum File Age

Each entry in the Destination File Table contains a maximum age value. This value represents the length of time, in seconds, that a particular data storage file may remain open.

As part of processing the housekeeping request command, DS checks the age of all open data storage files.

If the current file age exceeds the maximum age, the DS will close the file. A new file will be created only when another packet is received that passes the filter tests and targets that particular entry in the Destination File Table.

### Maximum File Size

Each entry in the Destination File Table contains a maximum file size value. This number represents the maximum file size, in bytes, for a particular data storage file.

Prior to writing a packet to an existing data storage file, DS performs a test to see if the current file size plus the size of the packet would exceed the maximum size for that particular file.

If the resulting file size would exceed the maximum file size, then DS will close the old file and open a new file before writing the packet data.

Note that there is no size test performed on the first packet written to a new data storage file. This scheme ensures that every packet can be written to a file and that there are no empty files, but at the cost that a file with a single large packet may exceed the size limit.

This page intentionally blank

# Frequently Asked Questions (FAQs)

## How do I downlink the files saved by DS?

DS has nothing to do with downlinking packets and files. A file delivery application such as the CFDP (CF) application is required to downlink the files created by DS.

## Are there any issues in limiting data?

One early task for FOT is to set up the Packet Filter Table to limit collection of data to the desired amount between downlinking times. To do this, FOT should understand the Packet Filter Table. Remember that the Destination File Table doesn’t have anything to do with limiting data. The Packet Filter Table alone “limits” the data.

## How can I keep files open?

There may arise a need to record all data when either not in contact with the ground, or when in contact, if the downlink rate is not high enough for all data. Later, at some point, it can be decided whether to downlink or delete the files.

There are no settings to keep files open indefinitely, but to effectively bypass size and age settings, these can be defined at the maximum value (4 billion hex), a value higher than either disc size or mission lifetime, respectively. The application will continue to check the values, but this setting will effectively keep the file open until manually closed by command.

This page intentionally blank

CFS DS Reference

HK Packet Telemetry

The telemetry in this section is contained in packets related to housekeeping.

Table Telemetry Data - Application State

|  |  |
| --- | --- |
| Name | AppEnableState |
| Description | AppEnableState denotes whether the DS application is enabled or disabled. |
| Data Type | Unsigned Eight Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_AppEnaState* |

Table Telemetry Data - Commands Accepted Counter

|  |  |
| --- | --- |
| Name | CmdAcceptedCounter |
| Description | CmdAcceptedCounter contains the count of valid commands received. |
| Data Type | Unsigned Eight Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_CMDPC* |

Table Telemetry Data - Commands Rejected Counter

|  |  |
| --- | --- |
| Name | CmdRejectedCounter |
| Description | CmdRejectedCounter contains the number of commands with process errors. |
| Data Type | Unsigned Eight Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_CMDEC* |

Table Telemetry Data - Destination Table Error Counter

|  |  |
| --- | --- |
| Name | DestTblErrCounter |
| Description | DestTblErrCounter contains the count of the number of times that cFE Table Services attempted and failed to get Destination File Table data. |
| Data Type | Unsigned Eight Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_DestPtrErrCnt* |

Table Telemetry Data – Count of Destination File Table Loads

|  |  |
| --- | --- |
| Name | DestTblLoadCounter |
| Description | DestTblLoadCounter contains the count of the number of times that cFE Table Services signaled new Destination File Table data. |
| Data Type | Unsigned Eight Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_DestLoadCnt* |

Table Telemetry Data - Count of Packets Discarded While DS Was Disabled

|  |  |
| --- | --- |
| Name | DisabledPktCounter |
| Description | DisabledPktCounter contains the count of the number of packets not processed because the packet processor was disabled. |
| Data Type | Unsigned 32 Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_DisabledPktCnt* |

Table Telemetry Data – Count of Good Updates to Secondary Header

|  |  |
| --- | --- |
| Name | FileUpdateCounter |
| Description | FileUpdateCounter contains the count of the number of files with the secondary header successfully updated prior to being closed. |
| Data Type | Unsigned 16 Bit IntegerUnsigned 16 Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpua\_DS\_FileUpdCnt* |

Table Telemetry Data – File Update Error Counter

|  |  |
| --- | --- |
| Name | FileUpdateErrCounter |
| Description | FileUpdateErrCounter contains the count of the number of errors generated while unsuccessfully attempting to update the secondary file header. |
| Data Type | Unsigned 16 Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DSFileUpdErrCnt* |

Table Telemetry Data – File Write Counter

|  |  |
| --- | --- |
| Name | FileWriteCounter |
| Description | FileWriteCounter contains the count of the total number of successful file writes. |
| Data Type | Unsigned 16 Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_FileWriteCnt* |

Table Telemetry Data - Total Number of File Write Errors

|  |  |
| --- | --- |
| Name | FileWriteErrCounter |
| Description | FileWriteErrCounter contains the count of the number of unsuccessful destination file writes. |
| Data Type | Unsigned 16 Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_FileWriteErrCnt* |

Table Telemetry Data - Filtered Packet Counter

|  |  |
| --- | --- |
| Name | FilteredPktCounter |
| Description | FilteredPktCounter contains a count of packets discarded, because they failed all filter tests, including because of disabled destination files. |
| Data Type | Unsigned 32 Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_FilteredPktCnt* |

Table Telemetry Data – Packet Filter Table Error Counter

|  |  |
| --- | --- |
| Name | FilterTblErrCounter |
| Description | FilterTblErrCounter contains the count of the number of times that cFE Table Services was unsuccessful in attempting to get Packet Filter Table data. |
| Data Type | Unsigned Eight Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_FilterPtrErrCnt* |

Table Telemetry Data – Packet Filter Table Load Counter

|  |  |
| --- | --- |
| Name | FilterTblLoadCounter |
| Description | FilterTblLoadCounter contains the count of the number of times that cFE Table Services signaled new Packet Filter Table data was available. |
| Data Type | Unsigned Eight Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_FilterLoadCnt* |

Table Telemetry Data - Count of Packets Discarded - Packet Has No Filter

|  |  |
| --- | --- |
| Name | IgnoredPktCounter |
| Description | IgnoredPktCounter contains the count of the number of packets not processed because tables were not loaded or because the packet was not in the Packet Filter Table. |
| Data Type | Unsigned 32 Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_IgnoredPktCnt* |

Table Telemetry Data - Passed Packet Counter

|  |  |
| --- | --- |
| Name | PassedPktCounter |
| Description | PassedPktCounter contains the count of the number of packets processed that passed at least one filter test. |
| Data Type | Unsigned 32 Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_PassedPktCnt* |

File Telemetry

The telemetry in this section is contained in packets related to file information.

Table Telemetry Data - File Enable State

|  |  |
| --- | --- |
| Name | EnableState |
| Description | EnableState contains the current state of the DS application. The possible states are enabled or disabled. |
| Data Type | Unsigned 16 Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_FileState[].EnableState* |

Table Telemetry Data - File Age

|  |  |
| --- | --- |
| Name | FileAge |
| Description | FileAge contains the current age of the file, in seconds. |
| Data Type | Unsigned 32 Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_FileState[].FileAge* |

Table Telemetry Data - Filename

|  |  |
| --- | --- |
| Name | FileName |
| Description | FileName contains the full filename of the file, if open. The full filename includes the Pathname, plus the Basename, plus a Sequence number, and finally, an extension.  Basename refers to the portion of the Data Storage filename that follows the pathname, and precedes the sequence number. Sequence number refers to a counter maintained by DS used to uniquely identify a file. |
| Data Type | Char |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_FileState[].FileName* |

Table Telemetry Data –File Rate of Growth

|  |  |
| --- | --- |
| Name | FileRate |
| Description | FileRate contains the average rate of growth of the current file in bytes per second since the last housekeeping request. |
| Data Type | Unsigned 32 Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_FileState[].FileRate* |

Table Telemetry Data – File Size

|  |  |
| --- | --- |
| Name | FileSize |
| Description | FileSize contains the size of the current file in bytes. |
| Data Type | Unsigned 32 Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_FileState[].FileSize* |

Table Telemetry Data – File Open State

|  |  |
| --- | --- |
| Name | OpenState |
| Description | OpenState contains the open or close state of the current file. |
| Data Type | Unsigned 16 Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_FileState[].OpenState* |

Table Telemetry Data - Filename Sequence Count

|  |  |
| --- | --- |
| Name | SequenceCount |
| Description | SequenceCount contains the sequence counter value that will be inserted into the filename of the next file to be created. |
| Data Type | Unsigned 32 Bit Integer |
| Telemetry Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_FileState[].FileSeq* |

Configuration Parameters

This section shows the DS Configuration Parameters provided as a default by the CFS DS application. Space is provided below for these values to be updated by the mission. If the mission has configured non-default values, they will be documented in the flight software RDL database.

While configuration parameters cannot be changed by the FOT, and are generally never changed after launch except by FSSE, the FOT needs to know the mission-specific values that have been incorporated into the software at the time the software was finalized and compiled.

(From an FSSE standpoint, configuration parameters are defined in the source code in ds\_platform\_cfg.h)

Table Configuration Parameter - Application Pipe Depth

|  |  |
| --- | --- |
| Configuration Parameter | DS\_APP\_PIPE\_DEPTH |
| Value | *CFS DS Default: 256* |
| Purpose | Application Pipe Depth |
| Description | * This parameter defines the depth of the DS input pipe. * The depth should be deep enough to accommodate all of the DS command packets and all of the subscribed telemetry packets that might be generated by applications with a priority higher than the DS application. |
| Limits | The value must be greater than zero and cannot exceed the definition of CFE\_SB\_MAX\_PIPE\_DEPTH. |

Table Configuration Parameter - Application Pipe Name

|  |  |
| --- | --- |
| Configuration Parameter | DS\_APP\_PIPE\_NAME |
| Value | *CFS DS Default: "DS\_CMD\_PIPE"* |
| Purpose | Application Pipe Name |
| Description | * This parameter defines a portion of the logical name used during the creation of the DS input pipe. * The logical name may also be used as an identifier when accessing status for the pipe via cFE Software Bus Services. * The entire logical name is "DS.DS\_CMD\_PIPE". |
| Limits | The string length (including string terminator) cannot exceed the maximum size allowed by the Operating System (OS) (OS\_MAX\_API\_NAME). The limit is not verified. |

Table Configuration Parameter - Destination File Table - Basename Buffer Size

|  |  |
| --- | --- |
| Configuration Parameter | DS\_BASENAME\_BUFSIZE |
| Value | *CFS DS Default: OS\_MAX\_PATH\_LEN* |
| Purpose | Destination File Table - Basename Buffer Size |
| Description | * This parameter further defines the size of the Destination File Table by setting the size of the basename buffer for each file entry. * Note that the buffer must contain both the string and the string terminator - so the max string length is one less than the buffer size. |
| Limits | * The buffer size must be greater than zero and a multiple of four bytes for alignment. * The value cannot exceed the maximum filename size allowed by the OS (OS\_MAX\_PATH\_LEN). |

Table Configuration Parameter - Destination File Table - Default Table Filename

|  |  |
| --- | --- |
| Configuration Parameter | DS\_DEF\_DEST\_FILENAME |
| Value | *CFS DS Default: "/cf/apps/ds\_file\_tbl.tbl"* |
| Purpose | Destination File Table - Default Table Filename |
| Description | This parameter defines the default filename for the Destination File Table. |
| Limits | The string length (including string terminator) cannot exceed the maximum filename size allowed by the OS [(OS\_MAX\_PATH\_LEN). The limit is not verified.] |

Table Configuration Parameter - Default DS Packet Processor State

|  |  |
| --- | --- |
| Configuration Parameter | DS\_DEF\_ENABLE\_STATE |
| Value | *CFS DS Default: 1* |
| Purpose | Default DS Packet Processor State |
| Description | * Set this parameter to a value of one and DS will begin to process packets immediately on startup. * Set the value to zero and DS will ignore data packets until receipt of a valid DS\_ENABLE command. |
| Limits | This parameter must be set to zero or one. |

Table Configuration Parameter - Packet Filter Table - Default Table Filename

|  |  |
| --- | --- |
| Configuration Parameter | DS\_DEF\_FILTER\_FILENAME |
| Value | *CFS DS Default: " /cf/apps/ds\_filter\_tbl.tbl"* |
| Purpose | Packet Filter Table - Default Table Filename |
| Description | This parameter defines the default filename for the Packet Filter Table. |
| Limits | The string length (including string terminator) cannot exceed the maximum filename size allowed by the OS [(OS\_MAX\_PATH\_LEN). The limit is not verified.] |

Table Configuration Parameter - Common Table File - Descriptor Text Buffer Size

|  |  |
| --- | --- |
| Configuration Parameter | DS\_DESCRIPTOR\_BUFSIZE |
| Value | *CFS DS Default: 32* |
| Purpose | Common Table File - Descriptor Text Buffer Size |
| Description | * This parameter defines the size of the Descriptor Text fields in both the Destination File Table and the Packet Filter Table. * The buffer includes the string terminator. |
| Limits | The buffer size must be greater than zero and a multiple of four bytes for alignment. There is no upper limit. |

Table Configuration Parameter - Destination File Table - Number of Files

|  |  |
| --- | --- |
| Configuration Parameter | DS\_DEST\_FILE\_CNT |
| Value | *CFS DS Default: 16* |
| Purpose | Destination File Table - Number of Files |
| Description | * This parameter defines the size of the DS Destination File Table by setting the number of file entries in the table. * The number should be large enough to provide an entry for all the destination files defined for the project. * Maintenance will be simplified if file index 'n' always describes the same file - even if that file is not in use at the present time. |
| Limits | The number must be greater than zero but there is no upper enforced limit for this parameter. |

Table Configuration Parameter - Destination File Table - Logical Table Name

|  |  |
| --- | --- |
| Configuration Parameter | DS\_DESTINATION\_TBL\_NAME |
| Value | *CFS DS Default: "FILE\_TBL"* |
| Purpose | Destination File Table - Logical Table Name |
| Description | * This parameter defines the name of the DS Destination File Table when referenced via cFE Table Services. * Note that this parameter is not a filename, but rather the table specific portion of the logical name. * The entire logical name for this table is "DS.FILE\_TBL". |
| Limits | The string length (including string terminator) cannot exceed the cFE configuration parameter CFE\_TBL\_MAX\_NAME\_LENGTH. The limit is not verified. |

Table Configuration Parameter - Destination File Table - Extension Buffer Size

|  |  |
| --- | --- |
| Configuration Parameter | DS\_EXTENSION\_BUFSIZE |
| Value | *CFS DS Default: 8* |
| Purpose | Destination File Table - Extension Buffer Size |
| Description | * This parameter further defines the size of the Destination File Table by setting the size of the extension buffer for each file entry. * Note that the buffer must contain both the string and the string terminator - so the max string length is one less than the buffer size. |
| Limits | * The buffer size must be greater than zero and a multiple of four bytes for alignment. * The value cannot exceed the maximum filename size allowed by the OS (OS\_MAX\_PATH\_LEN). |

Table Configuration Parameter - Data Storage File - cFE File Header Description

|  |  |
| --- | --- |
| Configuration Parameter | DS\_FILE\_HDR\_DESCRIPTION |
| Value | *CFS DS Default: "DS data storage file"* |
| Purpose | Data Storage File - cFE File Header Description |
| Description | This parameter defines a mission-specific text string that may be used to identify Data Storage files. |
| Limits | The string length including string terminator cannot exceed CFE\_FS\_HDR\_DESC\_MAX\_LEN. The limit is not verified. |

Table Configuration Parameter - Data Storage File - cFE File Header Sub-Type

|  |  |
| --- | --- |
| Configuration Parameter | DS\_FILE\_HDR\_SUBTYPE |
|  | *CFS DS Default: 12345* |
| Purpose | Data Storage File - cFE File Header Sub-Type |
| Description | This parameter defines a mission-specific value that is used to identify a Data Storage file. |
| Limits | The file header data type for the value is 32 bits unsigned, thus the value can be anything from zero to 4,294,967,295. The limit is not verified. |

Table Configuration Parameter - File Header Type Selection

|  |  |
| --- | --- |
| Configuration Parameter | DS\_FILE\_HEADER\_TYPE |
| Value | *CFS DS Default: 1* |
| Purpose | File Header Type Selection |
| Description | Set this parameter to select the type of file header that will be the first record written to each Data Storage File. |
| Limits | This parameter must be set to one of the following:   * 0 = none -- set this value to have no file header * 1 = CFE -- set this value to use cFE file headers * 2 = GPM -- set this value to use GPM file headers |

Table Configuration Parameter - Data Storage File - Minimum Age Limit

|  |  |
| --- | --- |
| Configuration Parameter | DS\_FILE\_MIN\_AGE\_LIMIT |
| Value | *CFS DS Default: 60* |
| Purpose | Data Storage File - Minimum Age Limit |
| Description | This parameter defines the lower limit for commands and table entries that define the age (in seconds) when a data storage file is automatically closed. |
| Limits | None.  **Caution:** A very small value will allow an age limit that closes files too frequently, while a very large value will effectively prevent files from ever being closed due to age. |

Table Configuration Parameter - Data Storage File - Minimum Size Limit

|  |  |
| --- | --- |
| Configuration Parameter | DS\_FILE\_MIN\_SIZE\_LIMIT |
| Value | *CFS DS Default: 1024* |
| Purpose | Data Storage File - Minimum Size Limit |
| Description | This parameter defines the lower limit for commands and table entries that define the size (in bytes) when a data storage file is automatically closed. |
| Limits | **Caution:** A very small value will allow a size limit that closes files too frequently, while a very large value will effectively prevent files from ever being closed due to size. |

Table Configuration Parameter - Packet Filter Table - Logical Table Name

|  |  |
| --- | --- |
| Configuration Parameter | DS\_FILTER\_TBL\_NAME |
| Value | *CFS DS Default: "FILTER\_TBL"* |
| Purpose | Packet Filter Table - Logical Table Name |
| Description | * This parameter defines the name of the DS Packet Filter Table when referenced via cFE Table Services. * Note that this parameter is not a filename. It is the table specific portion of the logical name. * The entire logical name for this table is "DS.FILTER\_TBL". |
| Limits | The string length (including string terminator) cannot exceed the cFE configuration parameter CFE\_TBL\_MAX\_NAME\_LENGTH. The limit is not verified. |

Table Configuration Parameter - Packet Filter Table - Filters Per Packet

|  |  |
| --- | --- |
| Configuration Parameter | DS\_FILTERS\_PER\_PACKET |
| Value | *CFS DS Default: 4* |
| Purpose | Packet Filter Table - Filters Per Packet |
| Description | * This parameter further defines the size of the DS Packet Filter Table by setting the number of filters per packet entry. * This is the maximum number of destination files to which a single packet can be written (at one time). |
| Limits | The number of filters per packet must be greater than zero and not greater than DS\_DEST\_FILE\_CNT. |

Table Configuration Parameter - Make DS Tables Critical

|  |  |
| --- | --- |
| Configuration Parameter | DS\_MAKE\_TABLES\_CRITICAL |
| Value | *CFS DS Default: 0* |
| Purpose | Make DS Tables Critical |
| Description | Set this parameter to a value of one to make the DS tables critical, otherwise set to zero. |
| Limits | This parameter must be set to zero or one. |

Table Configuration Parameter - Filename Sequence Count - Max Counter Value

|  |  |
| --- | --- |
| Configuration Parameter | DS\_MAX\_SEQUENCE\_COUNT |
| Value | *CFS DS Default: 99999999* |
| Purpose | Filename Sequence Count - Max Counter Value |
| Description | This parameter defines the maximum value a file sequence count will reach before rollover. |
| Limits | The value must be greater than zero and should not have more digits than the number of sequence count digits defined for DS\_SEQUENCE\_DIGITS, above. |

Table Configuration Parameter - Mission Specific Version Number for DS Application

|  |  |
| --- | --- |
| Configuration Parameter | DS\_MISSION\_REV |
| Value | *CFS DS Default: 0* |
| Purpose | Mission Specific Version Number for DS Application |
| Description | * An application version number consists of four parts: major version number, minor version number, revision number and mission specific revision number. * The mission specific revision number is defined here and the other parts are defined in "ds\_version.h". |
| Limits | Must be defined as a numeric value that is greater than or equal to zero. |

Table Configuration Parameter - Move Files to Downlink Directory After Close Selection

|  |  |
| --- | --- |
| Configuration Parameter | DS\_MOVE\_FILES |
| Value | *CFS DS Default: FALSE* |
| Purpose | Move Files to Downlink Directory After Close Selection |
| Description | * Set this parameter to enable the code and structures to automatically move DS files to another directory after closing the files. * The intended use for this setting is to move files from a working directory into a directory from which the files can be downlinked. * Note that even after enabling this feature, files will not be moved if the move pathname in the Destination File Table is null. |
| Limits | This parameter must be set to one of the following:   * TRUE = add move pathname field to Destination File Table. * FALSE = do not add move pathname to Destination File Table. |

Table Configuration Parameter - Packet Filter Table - Number of Packets

|  |  |
| --- | --- |
| Configuration Parameter | DS\_PACKETS\_IN\_FILTER\_TABLE |
| Value | *CFS DS Default: 256* |
| Purpose | Packet Filter Table - Number of Packets |
| Description | * This parameter defines the size of the DS Packet Filter Table by setting the number of packet entries in the table. * The number should be large enough to provide an entry for each command and telemetry packet subject to data storage. |
| Limits | * The number must be greater than zero but there is no upper enforced limit for this parameter. * CAUTION: Setting the size equal to the number of packets that might be subject to data storage, rather than the total number of packets defined for this project, will reduce the table file size, possibly significantly. |

Table Configuration Parameter - Destination File Table - Pathname Buffer Size

|  |  |
| --- | --- |
| Configuration Parameter | DS\_PATHNAME\_BUFSIZE |
| Value | *CFS DS Default: OS\_MAX\_PATH\_LEN* |
| Purpose | Destination File Table - Pathname Buffer Size |
| Description | * This parameter further defines the size of the Destination File Table by setting the size of the pathname buffer for each file entry. * Note that the buffer must contain both the string and the string terminator - so the max string length is one less than the buffer size. |
| Limits | * The buffer size must be greater than zero and a multiple of four bytes for alignment. * The value cannot exceed the maximum filename size allowed by the OS (OS\_MAX\_PATH\_LEN). |

Table Configuration Parameter - Application per Packet Pipe Limit

|  |  |
| --- | --- |
| Configuration Parameter | DS\_PER\_PACKET\_PIPE\_LIMIT |
| Value | *CFS DS Default: 50* |
| Purpose | Application per Packet Pipe Limit |
| Description | * This parameter defines the per packet pipe limit. * This is the max number of packets with the same Message ID that may be in the DS input pipe at any one time. * This value should be large enough to accommodate a burst of packets (usually event packets) plus a suitable margin. |
| Limits | The value must be greater than zero and cannot exceed the definition of DS\_APP\_PIPE\_DEPTH. |

Table Configuration Parameter - Housekeeping Request Frequency

|  |  |
| --- | --- |
| Configuration Parameter | DS\_SECS\_PER\_HK\_CYCLE |
| Value | *CFS DS Default: 4* |
| Purpose | Housekeeping Request Frequency |
| Description | * Set this parameter equal to the number of seconds between housekeeping request commands. * This number is mission specific and must match the frequency used by the source of the command - often the scheduler task. * The value is used by the DS application to measure file age and also as a factor in the calculation of file growth rates. |
| Limits | This parameter must be greater than zero. |

Table Configuration Parameter - Filename Sequence Count - Number of Digits

|  |  |
| --- | --- |
| Configuration Parameter | DS\_SEQUENCE\_DIGITS |
| Value | *CFS DS Default: 8* |
| Purpose | Filename Sequence Count - Number of Digits |
| Description | * This parameter defines the number of filename sequence count digits used when the filename type has been set to "count" rather than "time". * Sequence counts are padded with leading zero's to create fixed length strings. |
| Limits | * The number of sequence count digits must be greater than zero - even if there is no intention of later setting the filename type to "count". * This value should match the definition for DS\_MAX\_SEQUENCE\_COUNT, below. |

Table Configuration Parameter - Data Storage File - Total Filename Size

|  |  |
| --- | --- |
| Configuration Parameter | DS\_TOTAL\_FNAME\_BUFSIZE |
| Value | *CFS DS Default: OS\_MAX\_PATH\_LEN* |
| Purpose | Data Storage File - Total Filename Size |
| Description | This parameter defines the maximum size of a filename after combining the pathname, basename, sequence and extension. |
| Limits | * The buffer size must be greater than zero and a multiple of four bytes for alignment. * The buffer size (including string terminator) cannot exceed the value allowed by the OS (OS\_MAX\_PATH\_LEN). |

DS Commands

The tables in this section show detailed descriptions of all the standard commands available to ground controllers for use with the DS application.

Table Command 0 – No-op

|  |  |
| --- | --- |
| CFS DS Command Code | 0 |
| Command Name | No-Operation (No-op) Command |
| Description | * This command will increment the command execution counter and send an event containing the version number of the application. * The command is often used as a general test to verify the application is still "alive". |
| Command Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_NOOP* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * $sc\_$cpu\_DS\_CMDPC (or as defined by the mission) - command execution counter will increment * The Event ID 31 informational event message (No-op) will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * $sc\_$cpu\_DS\_CMDEC (or as defined by the mission) - command error counter will increment * The Event ID 32 error event message (No-op) will be sent |
| Criticality | None |

Table Command 1 – Reset Housekeeping Telemetry Counters

|  |  |
| --- | --- |
| CFS DS Command Code | 1 |
| Command Name | Reset Housekeeping Telemetry Counters Command |
| Description | The ability to reset the housekeeping counters is Important for testing and on orbit flight operations in order to start with a “clean slate”.  This command will set the following housekeeping counters to zero:   * Command Execution Counter *($sc\_$cpu\_DS\_CMDPC)\** * Command Error Counter *($sc\_$cpu\_DS\_CMDEC) \** * Ignored Packet Counter *($sc\_$cpu\_DS\_IgnoredPktCnt) \** * Filtered Packet Counter *($sc\_$cpu\_DS\_FilteredPktCnt) \** * Passed Packet Counter *($sc\_$cpu\_DS\_PassedPktCnt) \** * File Access Counter *($sc\_$cpu\_DS\_FileWriteCnt) \** * File Access Error Counter *($sc\_$cpu\_DS\_FileWriteErrCnt) \** * Destination Table Load Counter *($sc\_$cpu\_DS\_DestLoadCnt) \** * Filter Table Load Counter *($sc\_$cpu\_DS\_FilterLoadCnt) \** * Destination Table Pointer Error Counter *($sc\_$cpu\_DS\_DestPtrErrCnt) \** * Packet Filter Table Pointer Error Counter *($sc\_$cpu\_DS\_FilterPtrErrCnt) \**   *\* or as defined by the mission* |
| Command Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_ResetCtrs* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * *$sc\_$cpu\_DS\_CMDPC (or as defined by the mission)* - Command execution counter will increment * The Event ID 33 debug event message will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * *$sc\_$cpu\_DS\_CMDEC (or as defined by the mission)* - Command error counter will increment * The Event ID 34 error event message (Reset Housekeeping Counters) will be sent |
| Criticality | None |

Table Command 2 – Set Enable/Disable State For DS Application

|  |  |
| --- | --- |
| CFS DS Command Code | 2 |
| Command Name | Set Enable/Disable State For DS Application |
| Description | This command will modify the Enable/Disable State selection for the DS application. No packets are stored while DS is disabled.  The Disable command stops DS from filtering and storing messages. Since DS has multiple tables that are tightly coupled, FOT may use this command when needed to stop DS from new use of tables until all tables are updated. |
| Command Mnemonic(s) | *CFS DS Default:*   * *$sc\_$cpu\_DS\_Enable (fixed command arg = enable)* * *$sc\_$cpu\_DS\_Disable (fixed command arg = disable)* |
| Mission Specific Command Mnemonic(s) | Mission Defined |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * *$sc\_$cpu\_DS\_CMDPC (or as defined by the mission)* - Command execution counter will increment * The Event ID 35 debug event message will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length * Invalid enable/disable state selection |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * *$sc\_$cpu\_DS\_CMDEC (or as defined by the mission) -* Command error counter will increment * The Event ID 36 error event message (Set Application Enable/Disable State) will be sent |
| Criticality | **Potential flood of OS errors.**  FOT needs to ensure that the disk has been initialized and partitions created before enabling DS to avoid a flooding of OS errors when trying to create and write to files. |

Table Command 3 – Set Destination File For Packet Filter Table Entry

|  |  |
| --- | --- |
| CFS DS Command Code | 3 |
| Command Name | Set Destination File For Packet Filter Table Entry |
| Description | This command will modify the Destination File selection for the indicated entry in the Packet Filter Table. |
| Command Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_SetFilterFile* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * *$sc\_$cpu\_DS\_CMDPC (or as defined by the mission)* - Command execution counter will increment * The Event ID 37 debug event message will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length * Invalid Packet Filter Table index * Invalid filter parameters index * Invalid destination file selection * Packet Filter Table is not currently loaded * Cannot modify unused Packet Filter Table entry |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * *$sc\_$cpu\_DS\_CMDEC (or as defined by the mission)* - Command error counter will increment * The Event ID 38 error event message (Set Filter File Index) will be sent |
| Criticality | None |

Table Command 4 – Set Filter Type For Packet Filter Table Entry

|  |  |
| --- | --- |
| CFS DS Command Code | 4 |
| Command Name | Set Filter Type For Packet Filter Table Entry |
| Description | This command will modify the Filter Type selection for the indicated entry in the Packet Filter Table. |
| Command Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_SetFilterType* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * *$sc\_$cpu\_DS\_CMDPC (or as defined by the mission)* - Command execution counter will increment * The DS\_FTYPE\_CMD\_EID debug event message will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length * Invalid Packet Filter Table index * Invalid filter parameters index * Invalid filter type selection * Packet Filter Table is not currently loaded * Cannot modify unused Packet Filter Table entry |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * *$sc\_$cpu\_DS\_CMDEC (or as defined by the mission)* - Command error counter will increment * The Event ID 40 error event message (Set Filter Type) will be sent |
| Criticality | None |

Table Command 5 – Set Algorithm Parameters For Packet Filter Table Entry

|  |  |
| --- | --- |
| CFS DS Command Code | DS\_SET\_FILTER\_PARMS\_CC 5 |
| Command Name | Set Algorithm Parameters For Packet Filter Table Entry |
| Description | This command will modify the Algorithm Parameters for the indicated entry in the Packet Filter Table. |
| Command Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_SetFilterParams* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * $sc\_$cpu\_DS\_CMDPC (or as defined by the mission) - command execution counter will increment * The Event ID 41 debug event message will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length * Invalid Packet Filter Table index * Invalid filter parameters index * Algorithm\_N value cannot be greater than Algorithm\_X * Packet Filter Table is not currently loaded * Cannot modify unused Packet Filter Table entry |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * $sc\_$cpu\_DS\_CMDEC (or as defined by the mission) - command error counter will increment * The Event ID 42 error event message (Set Filter Parameters) will be sent |
| Criticality | None |

Table Command 6 – Set Filename Type For Destination File Table Entry

|  |  |
| --- | --- |
| CFS DS Command Code | 6 |
| Command Name | Set Filename Type For Destination File Table Entry |
| Description | This command will modify the Filename Type selection for the indicated entry in the Destination File Table. |
| Command Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_SetFileType* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * $sc\_$cpu\_DS\_CMDPC (or as defined by the mission) - command execution counter will increment * The Event ID 43 debug event message will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length * Invalid Destination File Table index * Invalid filename type selection * Destination File Table is not currently loaded |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * $sc\_$cpu\_DS\_CMDEC (or as defined by the mission) - command error counter will increment * The Event ID 44 error event message (Set Filename Type) will be sent |
| Criticality | None |

Table Command 7 – Set Enable/Disable State For Destination File Table Entry

|  |  |
| --- | --- |
| CFS DS Command Code | 7 |
| Command Name | Set Enable/Disable State For Destination File Table Entry |
| Description | This command will modify the Enabled/Disabled State selection for the indicated entry in the Destination File Table.  The enabled state provides the ground the ability to write files in a file set without having to load a table.  The disabled state provides ground ability to quickly stop writing files in a file set without having to load a table. |
| Command Mnemonic(s) | *CFS DS Default*   * *$sc\_$cpu\_DS\_EnableFile (fixed command arg = enable)* * *$sc\_$cpu\_DS\_DisableFile (fixed command arg = disable)* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * *$sc\_$cpu\_DS\_CMDPC (or as defined by the mission)* - Command execution counter will increment * The Event ID 45 debug event message will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length * Invalid Destination File Table index * Invalid destination state selection * Destination File Table is not currently loaded |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * *$sc\_$cpu\_DS\_CMDEC (or as defined by the mission)* - Command error counter will increment * The Event ID 46 error event message (Set File Enable/Disable State) will be sent |
| Criticality | **Potential packet loss.**  It is the responsibility of the user to verify the FileID specifying the destination to be disabled. The user should use caution when issuing this command. |

Table Command 8 – Set Pathname For Destination File Table Entry

|  |  |
| --- | --- |
| CFS DS Command Code | 8 |
| Command Name | Set Pathname For Destination File Table Entry |
| Description | This command will modify the Pathname portion of the filename for the indicated entry in the Destination File Table. |
| Command Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_SetPath* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * *$sc\_$cpu\_DS\_CMDPC (or as defined by the mission)* - Command execution counter will increment * The Event ID 47 debug event message will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length * Invalid Destination File Table index * Invalid pathname string (empty, no terminator, bad characters) * Destination File Table is not currently loaded |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * *$sc\_$cpu\_DS\_CMDEC (or as defined by the mission)* - Command error counter will increment * The Event ID 48 error event message (Set Filename Path) will be sent |
| Criticality | **Potential packet loss.**  It is the responsibility of the user to verify the new Pathname and ensure it is a valid path. The user should use caution when issuing this command. |

Table Command 9 – Set Basename For Destination File Table Entry

|  |  |
| --- | --- |
| CFS DS Command Code | 9 |
| Command Name | Set Basename For Destination File Table Entry |
| Description | This command will modify the Basename portion of the filename for the indicated entry in the Destination File Table.   * This command affects the next file opened in the File Set. * This command does not affect the File Sequence Counter. |
| Command Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_SetBaseName* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * *$sc\_$cpu\_DS\_CMDPC (or as defined by the mission)* - Command execution counter will increment * The Event ID 49 debug event message will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length * Invalid Destination File Table index * Invalid basename string (no terminator, bad characters) * Destination File Table is not currently loaded |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * *$sc\_$cpu\_DS\_CMDEC (or as defined by the mission)* - Command error counter will increment * The Event ID 50 error event message (Set File Basename) will be sent |
| Criticality | None |

Table Command 10 – Set Extension For Destination File Table Entry

|  |  |
| --- | --- |
| CFS DS Command Code | 10 |
| Command Name | Set Extension For Destination File Table Entry |
| Description | This command will modify the Extension portion of the filename for the indicated entry in the Destination File Table. |
| Command Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_SetExtension* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * *$sc\_$cpu\_DS\_CMDPC (or as defined by the mission)* - Command execution counter will increment * The Event ID 51 debug event message will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length * Invalid Destination File Table index * Invalid extension string (empty, no terminator, bad characters) * Destination File Table is not currently loaded |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * *$sc\_$cpu\_DS\_CMDEC (or as defined by the mission)* - Command error counter will increment * The Event ID 52 error event message (Set Filename Extension) will be sent |
| Criticality | None |

Table Command 11 – Set Max File Size For Destination File Table Entry

|  |  |
| --- | --- |
| CFS DS Command Code | 11 |
| Command Name | Set Max File Size For Destination File Table Entry |
| Description | This command will modify the max file size selection for the indicated entry in the Destination File Table. |
| Command Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_SetMaxFileSize* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * *$sc\_$cpu\_DS\_CMDPC (or as defined by the mission)* - Command execution counter will increment * The Event ID 53 debug event message will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length * Invalid Destination File Table index * Invalid max file size selection * Destination File Table is not currently loaded |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * *$sc\_$cpu\_DS\_CMDEC (or as defined by the mission) -* Command error counter will increment * The Event ID 54 error event message (Set Max File Size) will be sent |
| Criticality | **Potential to fill the storage device and/or hog CPU.**  Downlinking many small files can be CPU intensive. It is the responsibility of the user to verify the File Size. The user should use caution when issuing this command. |

Table Command 12 – Set Max File Age For Destination File Table Entry

|  |  |
| --- | --- |
| CFS DS Command Code | 12 |
| Command Name | Set Max File Age For Destination File Table Entry |
| Description | This command will modify the max file age selection for the indicated entry in the Destination File Table. |
| Command Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_SetMaxFileAge* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * *$sc\_$cpu\_DS\_CMDPC (or as defined by the mission)* - Command execution counter will increment * The Event ID 55 debug event message will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length * Invalid Destination File Table index * Invalid max file age selection * Destination File Table is not currently loaded |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * *$sc\_$cpu\_DS\_CMDEC (or as defined by the mission)* - Command error counter will increment * The Event ID 56 error event message (Set Max File Age) will be sent |
| Criticality | **Potential to fill the storage device and/or hog CPU.**  Downlinking many small files can be CPU intensive. It is the responsibility of the user to verify the File Size. The user should use caution when issuing this command. |

Table Command 13 – Set Sequence Count For Destination File Table Entry

|  |  |
| --- | --- |
| CFS DS Command Code | DS\_SET\_DEST\_COUNT\_CC 13 |
| Command Name | Set Sequence Count For Destination File Table Entry |
| Description | This command will modify the sequence count value for the indicated entry in the Destination File Table.   * Use of this command affects the next file opened in the File Set. * This command does not affect the File Sequence Counter. * This command could be used in the event of a power-on reset so that sequence numbers continue. * However, in a cFE Processor reset, use of the command for this purpose should be unnecessary because the sequence numbers should already be preserved. |
| Command Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_SetFileSeqCtr* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * *$sc\_$cpu\_DS\_CMDPC (or as defined by the mission)* - Command execution counter will increment * The Event ID 57 debug event message will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length * Invalid Destination File Table index * Invalid sequence count value * Destination File Table is not currently loaded |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * *$sc\_$cpu\_DS\_CMDEC (or as defined by the mission)* - Command error counter will increment * The Event ID 58 error event message (Set Sequence Count) will be sent |
| Criticality | None |

Table Command 14 – Close Destination File

|  |  |
| --- | --- |
| CFS DS Command Code | DS\_CLOSE\_FILE\_CC 14 |
| Command Name | Close Destination File |
| Description | This command will close the indicated Destination File so that it can be downlinked. |
| Command Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_CloseFile* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * *$sc\_$cpu\_DS\_CMDPC (or as defined by the mission)* - Command execution counter will increment * The Event ID 59 debug event message will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length * Invalid Destination File Table index * Destination File Table is not currently loaded |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * *$sc\_$cpu\_DS\_CMDEC (or as defined by the mission)* - Command error counter will increment * The Event ID 60 error event message (Close Destination File) will be sent |
| Criticality | None |

Table Command 15 – Get File Info Packet

|  |  |
| --- | --- |
| CFS DS Command Code | 15 |
| Command Name | Get File Info Packet |
| Description | This command will send the DS File Info Packet. |
| Command Mnemonic(s) | *CFS DS Default: (N/A)* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * *$sc\_$cpu\_DS\_CMDPC (or as defined by the mission)* - Command execution counter will increment * The DS\_FileInfoPkt\_t packet will be sent |
| Error Condition | This command may fail for the following reason(s):   * Invalid command packet length |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * *$sc\_$cpu\_DS\_CMDEC (or as defined by the mission)* - Command error counter will increment * The Event ID 63 error event message (Get File Info) will be sent |
| Criticality | None |

Table Command 16 – Add Message ID to Packet Filter Table

|  |  |
| --- | --- |
| CFS DS Command Code | 16 |
| Command Name | Add Message ID To Packet Filter Table |
| Description | This command will change the Message ID selection for an unused Packet Filter Table entry to the indicated value. |
| Command Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_AddMID* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * *$sc\_$cpu\_DS\_CMDPC (or as defined by the mission)* - Command execution counter will increment * The Event ID 64 debug event message will be sent |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length * Message ID is invalid (can be anything but zero) * Packet Filter Table is not currently loaded * Message ID already exists in Packet Filter Table |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * *$sc\_$cpu\_DS\_CMDEC (or as defined by the mission)* - Command error counter will increment * The Event ID 65 error event message (Add Message ID to Packet Filter Table) will be sent |
| Criticality | None |

Table Command 17 – Close All Destination Files

|  |  |
| --- | --- |
| CFS DS Command Code | 17 |
| Command Name | Close All Destination Files |
| Description | * This command will close all open Destination Files. * NOTE: Using this command may incur a performance hit based upon the number and size of the files being closed. |
| Command Mnemonic(s) | *CFS DS Default: $sc\_$cpu\_DS\_CloseAll* |
| Command Verification | Successful execution of this command may be verified with the following telemetry:   * *$sc\_$cpu\_DS\_CMDPC (or as defined by the mission)* - Command execution counter will increment * The Event ID 66 debug event message will be sent (before launch, when debug events are generally turned off) |
| Error Conditions | This command may fail for the following reason(s):   * Invalid command packet length * Destination File Table is not currently loaded |
| Failure Evidence | Evidence of failure may be found in the following telemetry:   * *$sc\_$cpu\_DS\_CMDEC (or as defined by the mission)* - Command error counter will increment * The Event ID 67 error message will be sent |
| Criticality | None |

Event Messages

This section shows cFE Software Bus event messages. Event messages are not mission specific. Generally, if supported by ground flight software systems (e.g., ASIST or ITOS), the Event ID numbers shown in the subsections below should appear in telemetry, no matter the mission.

Event Messages - Critical

The tables in this section show **critical** event messages for the DS application.

Table Event ID 3 (Critical) - Application Termination

|  |  |
| --- | --- |
| Event ID Number | 3 |
| Event Name | 'Application Termination Event' |
| Event Message | 'Application terminating, err = 0x%08X' |
| Type | CRITICAL |
| Cause | * This event message is issued when the application performs a voluntary termination. The termination may be caused by a cFE command requesting the application be terminated - or, the cause may result from the DS application having received an error when invoking a cFE or operating system (OS) function necessary for normal operation. * The value displayed is either zero (if cFE requested the termination) or the return code from the function that failed. |

Event Messages - Error

The tables in this section show **error** event messages for the DS application.

Table Event ID 2 (Error) - Application Initialization

|  |  |
| --- | --- |
| Event ID Number | 2 |
| Event Name | 'Application Initialization (error)' |
| Event Message | * 'Unable to register for EVS services, err = 0x%08X' * 'Unable to create input pipe, err = 0x%08X' * 'Unable to subscribe to housekeeping request commands, err = 0x%08X' * 'Unable to subscribe to 1Hz wakeup commands, err = 0x%08X' * 'Unable to subscribe to DS commands, err = 0x%08X' |
| Type | ERROR |
| Cause | * This event message is issued when the application receives an error while performing cFE initialization. * The value displayed is the return code from the function that failed. |

Table Event ID 6 (Error) - Critical Data Store Access

|  |  |
| --- | --- |
| Event ID Number | 6 |
| Event Name | 'Critical Data Store Access (error)' |
| Event Message | 'Critical Data Store access error = 0x%08X' |
| Type | ERROR |
| Cause | * The DS application stores the current values for Destination Filename sequence counts in the CDS. This ensures that DS will not overwrite old data storage files following a processor reset. * This event indicates an error at startup as DS is initializing access to the CDS. Subsequent CDS errors are ignored by DS. |

Table Event ID 8 (Error) - Table Create

|  |  |
| --- | --- |
| Event ID Number | 8 |
| Event Name | 'Table Create (error)’ |
| Event Message | * 'Unable to register Filter Table: Error = 0x%08X' * 'Unable to register Destination File Table: Error = 0x%08X' * 'Unable to load default Destination File Table: Filename = '%s', Error = 0x%08X' * 'Unable to load default Filter Table: Filename = '%s', Error = 0x%08X' |
| Type | ERROR |
| Cause | * At startup, the DS application must create both a Packet Filter Table and a Destination File Table. After creating the tables, DS must then load default table data for each of the files. If DS is unable to create either table then the application will terminate. If DS is able to create both tables and is then unable to load both tables then DS will operate in a reduced function mode - thus allowing table load error recovery via the cFE Table Services command interface. * The values displayed indicate the cFE Table Services API function return code and the table filename, if appropriate. |

Table Event ID 11 (Error) - Destination File Validation

|  |  |
| --- | --- |
| Event ID Number | 11 |
| Event Name | 'Destination File Validation (error)’ |
| Event Message | * 'Destination file table verify err: invalid descriptor text' * 'Destination file table verify err: index = %d, invalid pathname text' * 'Destination file table verify err: index = %d, invalid basename text' * 'Destination file table verify err: index = %d, invalid extension text' * 'Destination file table verify err: index = %d, filename type = %d' * 'Destination file table verify err: index = %d, file enable state = %d' * 'Destination file table verify err: index = %d, max file size = %d' * 'Destination file table verify err: index = %d, max file age = %d' * 'Destination file table verify err: index = %d, sequence count = %d' |
| Type | ERROR |
| Cause | * These are the errors that the DS application might encounter when verifying the contents of a Destination File Table. Note that only the first error detected for each table file will result in an event being generated. The remaining entries are still tested to establish the result counters but no further error events will be generated during this call to the verify function. * The event text will indicate the table index value (where appropriate), the invalid field name and the field value for non-string fields. If a string field is invalid then attempts to display the string could result in other errors. |

Table Event ID 13 (Error) – Packet Filter Table Validation

|  |  |
| --- | --- |
| Event ID Number | 13 |
| Event Name | 'Packet Filter Table Validation (error)' |
| Event Messages | * 'Filter table verify err: invalid descriptor text' * 'Filter table verify err: MID = 0x%04X, index = %d, filter = %d, file table index = %d' * 'Filter table verify err: MID = 0x%04X, index = %d, filter = %d, filter type = %d' * 'Filter table verify err: MID = 0x%04X, index = %d, filter = %d, filter parms N = %d, X = %d, O = %d' |
| Type | ERROR |
| Cause | * These are the errors that the DS application might encounter when verifying the contents of a Packet Filter Table. Note that only the first error detected for each table file will result in an event being generated. The remaining entries are still tested to establish the result counters but no further error events will be generated during this call to the verify function. * The event text will indicate the Message ID, table index value and filter index value (where appropriate), the field name and the field value for non-string fields. If a string field is invalid then attempts to display the string could result in other errors. |

Table Event ID 14 (Error) - Filename Create

|  |  |
| --- | --- |
| Event ID Number | 14 |
| Event Name | 'Filename Create (error)' |
| Event Message | 'FILE NAME error: dest = %d, path = '%s', base = '%s', seq = '%s', ext = '%s'' |
| Type | ERROR |
| Cause | * This error occurs when an attempt to create a destination filename fails. The expected cause of this error is for the sum of the lengths of each filename element to be invalid, even though each individual element length is valid. Note that each of the individual element strings has been previously verified. * The event text will indicate the Destination File Table index, the file path string, the file basename string, the filename sequence string and the extension portion of the filename. * Note that the filename create error handler will also disable the destination to prevent the immediate re-occurrence of the error as more packets are written to this destination. |

Table Event ID 15 (Error) - File Create

|  |  |
| --- | --- |
| Event ID Number | 15 |
| Event Name | 'File Create (error)' |
| Event Message | 'FILE CREATE error: result = %d, dest = %d, name = '%s'' |
| Type | ERROR |
| Cause | * This error occurs when an attempt to create a destination file fails. The most common cause of this error is insufficient free space available on the target file system (disk). However, it is possible to specify a filename that is legal but still invalid (i.e. the path string has legal chars but does not exist). * The event text will indicate the result from the system function call to create the file, the Destination File Table index and the filename. * Note that the file create error handler will also disable the destination to prevent the immediate re-occurrence of the error as more packets are written to this destination. |

Table Event ID 16 (Error) - File Write

|  |  |
| --- | --- |
| Event ID Number | 16 |
| Event Name | ‘File Write (error)' |
| Event Message | ‘FILE WRITE error: result = %d, length = %d, dest = %d, name = '%s'' |
| Type | ERROR |
| Cause | * This error occurs when an attempt to write to a destination file fails. * The most common cause of this error is insufficient free space available on the target file system (disk). Other causes for this error imply some sort of operational or file system failure and will require careful analysis. * The event text will indicate the result from the system function call to write to the file, the Destination File Table index and the filename. * Note that the file write error handler will also close the file and disable the destination to prevent the immediate re-occurrence of the error as more packets are written to this destination. |

Table Event ID 21 (Error) - Invalid Packet

|  |  |
| --- | --- |
| Event ID Number | 21 |
| Event Name | 'Invalid Packet (command code)' |
| Event Message | 'Invalid command code: MID = 0x%04X, CC = %d' |
| Type | ERROR |
| Cause | * This error occurs when a DS application command is received that has an undefined command code (CC). Ground systems generally prevent these errors so the cause is more likely to result from sending "raw" ground commands or on-board stored commands. * The event text will indicate the Message ID (MID) and command code. |

Table Event ID 22 (Error) - Housekeeping Request

|  |  |
| --- | --- |
| Event ID Number | 22 |
| Event Name | 'Housekeeping Request (error)' |
| Event Message | 'Invalid HK request length: expected = %d, actual = %d' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a HK request command. * The cause of the failure is an invalid command packet length. |

Table Event ID 32 (Error) - No-op

|  |  |
| --- | --- |
| Event ID Number | 32 |
| Event Name | 'No-op command (error)' |
| Event Message | 'Invalid NOOP command length: expected = %d, actual = %d' |
| Type | ERROR |
| Cause | This event signals the failed execution of a NOOP command. The cause of the failure is an invalid command packet length. |

Table Event ID 34 (Error) - Reset Housekeeping Counters

|  |  |
| --- | --- |
| Event ID Number | 34 |
| Event Name | 'Reset Housekeeping Counters command (error)' |
| Event Message | 'Invalid RESET command length: expected = %d, actual = %d' |
| Type | ERROR |
| Cause | This event signals the failed execution of a RESET command. The cause of the failure is an invalid command packet length. |

Table Event ID 36 (Error) - Set Application Enable/Disable State

|  |  |
| --- | --- |
| Event ID Number | 36 |
| Event Name | 'Set Application Enable/Disable State Command (error)' |
| Event Message | * 'Invalid APP STATE command length: expected = %d, actual = %d' * 'Invalid APP STATE command arg: app state = %d' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a command to set the application enable/disable state. The cause of the failure may be an invalid command packet length or an invalid enable/disable state value. * The event text will indicate the cause of the failure. |

Table Event ID 38 (Error) - Set Filter File Index

|  |  |
| --- | --- |
| Event ID Number | 38 |
| Event Name | 'Set Filter File Index command (error)' |
| Event Message | * 'Invalid FILTER FILE command length: expected = %d, actual = %d' * 'Invalid FILTER FILE command arg: invalid messageID = 0x%04X' * 'Invalid FILTER FILE command arg: filter parameters index = %d' * 'Invalid FILTER FILE command arg: file table index = %d' * 'Invalid FILTER FILE command: packet filter table is not loaded' * 'Invalid FILTER FILE command: Message ID 0x%04X is not in filter table' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a command to set the Destination File Table index for a Packet Filter Table entry. The cause of the failure may be an invalid command packet length, an invalid Message ID or an invalid filter parameters index. * The failure may also result from not having a Packet Filter Table loaded at the time the command was invoked or because the Message ID was not found in the Packet Filter Table. * The event text will indicate the cause of the failure. |

Table Event ID 40 (Error) - Set Filter Type

|  |  |
| --- | --- |
| Event ID Number | 40 |
| Event Name | 'Set Filter Type command (error)' |
| Event Message | * 'Invalid FILTER TYPE command length: expected = %d, actual = %d' * 'Invalid FILTER TYPE command arg: invalid messageID = 0x%04X' * 'Invalid FILTER TYPE command arg: filter parameters index = %d' * 'Invalid FILTER TYPE command arg: filter type = %d' * 'Invalid FILTER TYPE command: packet filter table is not loaded' * 'Invalid FILTER TYPE command: Message ID 0x%04X is not in filter table' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a command to set the filter type for a Packet Filter Table entry. The cause of the failure may be an invalid command packet length, an invalid Message ID, an invalid Filter Parameters index or an invalid filter type. * The failure may also result from not having a Packet Filter Table loaded at the time the command was invoked or because the Message ID was not found in the Packet Filter Table. * The event text will indicate the cause of the failure. |

Table Event ID 42 (Error) - Set Filter Parameters

|  |  |
| --- | --- |
| Event ID Number | 42 |
| Event Name | 'Set Filter Parameters command (error)' |
| Event Message | * 'Invalid FILTER PARMS command length: expected = %d, actual = %d' * 'Invalid FILTER PARMS command arg: invalid messageID = 0x%04X' * 'Invalid FILTER PARMS command arg: filter parameters index = %d' * 'Invalid FILTER PARMS command arg: N = %d, X = %d, O = %d' * 'Invalid FILTER PARMS command: packet filter table is not loaded' * 'Invalid FILTER PARMS command: Message ID 0x%04X is not in filter table' |
| Type | ERROR3 |
| Cause | * This event signals the failed execution of a command to set the filter parameters for a Packet Filter Table entry. The cause of the failure may be an invalid command packet length, an invalid Message ID, an invalid filter parameters index or an invalid filter parameters value (N,X,O). * The failure may also result from not having a Packet Filter Table loaded at the time the command was invoked or because the Message ID was not found in the Packet Filter Table. * The event text will indicate the cause of the failure. |

Table Event ID 44 (Error) - Set Filename Type

|  |  |
| --- | --- |
| Event ID Number | 44 |
| Event Name | 'Set Filename Type command (error)' |
| Event Message | * 'Invalid DEST TYPE command length: expected = %d, actual = %d' * 'Invalid DEST TYPE command arg: file table index = %d' * 'Invalid DEST TYPE command arg: filename type = %d' * 'Invalid DEST TYPE command: destination file table is not loaded' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a command to set the filename type for the selected Destination File Table entry. The cause of the failure may be an invalid command packet length, an invalid Destination File Table index or an invalid filename type. * The failure may also result from not having a Destination File Table loaded at the time the command was invoked. * The event text will indicate the cause of the failure. |

Table Event ID 46 (Error) - Set File Enable/Disable State

|  |  |
| --- | --- |
| Event ID Number | 46 |
| Event Name | 'Set File Enable/Disable State command (error)' |
| Event Message | * 'Invalid DEST STATE command length: expected = %d, actual = %d' * 'Invalid DEST STATE command arg: file table index = %d' * ‘Invalid DEST STATE command arg: file state = %d' * ‘Invalid DEST STATE command: destination file table is not loaded' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a command to set the enable/disable state for the selected Destination File Table entry. The cause of the failure may be an invalid command packet length, an invalid Destination File Table index or an invalid state selection. * The failure may also result from not having a Destination File Table loaded at the time the command was invoked. * The event text will indicate the cause of the failure. |

Table Event ID 48 (Error) - Set Filename Path

|  |  |
| --- | --- |
| Event ID Number | 48 |
| Event Name | 'Set Filename Path command (error)' |
| Event Message | * 'Invalid DEST PATH command length: expected = %d, actual = %d' * 'Invalid DEST PATH command arg: file table index = %d' * 'Invalid DEST PATH command arg: pathname' * 'Invalid DEST PATH command: destination file table is not loaded' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a command to set the filename path text for a Destination File Table entry. The cause of the failure may be an invalid command packet length, an invalid Destination File Table index or invalid filename path text. * The failure may also result from not having a Destination File Table loaded at the time the command was invoked. * The event text will indicate the cause of the failure. |

Table Event ID 50 (Error) - Set File Basename

|  |  |
| --- | --- |
| Event ID Number | 50 |
| Event Name | 'Set File Basename command (error)' |
| Event Message | * 'Invalid DEST BASE command length: expected = %d, actual = %d' * 'Invalid DEST BASE command arg: file table index = %d' * 'Invalid DEST BASE command arg: base filename' * 'Invalid DEST BASE command: destination file table is not loaded' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a command to set the base filename text for a Destination File Table entry. The cause of the failure may be an invalid command packet length, an invalid Destination File Table index or invalid base filename text. * The failure may also result from not having a Destination File Table loaded at the time the command was invoked. * The event text will indicate the cause of the failure. |

Table Event ID 52 (Error) - Set Filename Extension

|  |  |
| --- | --- |
| Event ID Number | 52 |
| Event Name | 'Set Filename Extension command (error)' |
| Event Message | * 'Invalid DEST EXT command length: expected = %d, actual = %d' * 'Invalid DEST EXT command arg: file table index = %d' * 'Invalid DEST EXT command arg: extension' * 'Invalid DEST EXT command: destination file table is not loaded' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a command to set the filename extension text for a Destination File Table entry. The cause of the failure may be an invalid command packet length, an invalid Destination File Table index or invalid filename extension text. * The failure may also result from not having a Destination File Table loaded at the time the command was invoked. * The event text will indicate the cause of the failure. |

Table Event ID 54 (Error) - Set Max File Size

|  |  |
| --- | --- |
| Event ID Number | 54 |
| Event Name | 'Set Max File Size command (error)' |
| Event Message | * 'Invalid DEST SIZE command length: expected = %d, actual = %d' * 'Invalid DEST SIZE command arg: file table index = %d' * 'Invalid DEST SIZE command arg: size limit = %d' * 'Invalid DEST SIZE command: destination file table is not loaded' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a command to set the file size limit for a Destination File Table entry. The cause of the failure may be an invalid command packet length, an invalid Destination File Table index or an invalid file size limit. * The failure may also result from not having a Destination File Table loaded at the time the command was invoked. * The event text will indicate the cause of the failure. |

Table Event ID 55 (Error) - Set Max File Age

|  |  |
| --- | --- |
| Event ID Number | 55 |
| Event Name | 'Set Max File Age command (error)' |
| Event Message | 'DEST AGE command: file table index = %d, age limit = %d' |
| Type | DEBUG |
| Cause | * This event signals the successful execution of a command to set the file age limit for a Destination File Table entry. * The event text will indicate the Destination File Table index, and the new file age limit. |

Table Event ID 56 (Error) - Set Max File Age

|  |  |
| --- | --- |
| Event ID Number | 56 |
| Event Name | 'Set Max File Age command (error)' |
| Event Message | * 'Invalid DEST AGE command length: expected = %d, actual = %d' * 'Invalid DEST AGE command arg: file table index = %d' * 'Invalid DEST AGE command arg: age limit = %d' * 'Invalid DEST AGE command: destination file table is not loaded' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a command to set the file age limit for a Destination File Table entry. The cause of the failure may be an invalid command packet length, an invalid Destination File Table index or an invalid file age limit. * The failure may also result from not having a Destination File Table loaded at the time the command was invoked. * The event text will indicate the cause of the failure. |

Table Event ID 58 (Error) - Set Sequence Count

|  |  |
| --- | --- |
| Event ID Number | 58 |
| Event Name | 'Set Sequence Count command (error)' |
| Event Message | * 'Invalid DEST COUNT command length: expected = %d, actual = %d' * 'Invalid DEST COUNT command arg: file table index = %d' * 'Invalid DEST COUNT command arg: sequence count = %d' * 'Invalid DEST COUNT command: destination file table is not loaded' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a command to set the sequence count for a Destination File Table entry. The cause of the failure may be an invalid command packet length, an invalid Destination File Table index or an invalid sequence count. * The failure may also result from not having a Destination File Table loaded at the time the command was invoked. * The event text will indicate the cause of the failure. |

Table Event ID 60 (Error) - Close Destination File

|  |  |
| --- | --- |
| Event ID Number | 60 |
| Event Name | 'Close Destination File command (error)' |
| Event Message | * 'Invalid DEST CLOSE command length: expected = %d, actual = %d' * 'Invalid DEST CLOSE command arg: file table index = %d' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a command to close the selected Destination File. The cause of the failure may be an invalid command packet length or an invalid Destination File Table index. * The event text will indicate the cause of the failure. |

Table Event ID 61 (Error) - File Move

|  |  |
| --- | --- |
| Event ID Number | 61 |
| Event Name | 'File Move (error)’ |
| Event Message | * 'FILE MOVE error: dir name = '%s', filename = '%s'' * 'FILE MOVE error: src = '%s', tgt = '%s', result = %d' |
| Type | ERROR |
| Cause | * This event signals the failed attempt to move a Data Storage file from the temporary working directory it was created in, to the directory specified in the file definition table. The cause of the failure may be an invalid combined directory and filename length or the system file move function may have returned an error result. * The event text will indicate the cause of the failure. |

Table Event ID 63 (Error) - Get File Info

|  |  |
| --- | --- |
| Event ID Number | 63 |
| Event Name | 'Get File Info command (error)' |
| Event Message | 'Invalid GET FILE INFO command length: expected = %d, actual = %d' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a command to get the file info diagnostic packet. The cause of the failure is an invalid command packet length. * The event text will indicate the expected and actual packet size. |

Table Event ID 65 (Error) - Add Message ID to Packet Filter Table

|  |  |
| --- | --- |
| Event ID Number | 65 |
| Event Name | 'Add Message ID to Packet Filter Table command (error)' |
| Event Message | * 'Invalid ADD MID command length: expected = %d, actual = %d' * 'Invalid ADD MID command arg: invalid MID = 0x%4X' * 'Invalid ADD MID command: filter table is not loaded' * 'Invalid ADD MID command: MID = 0x%4X is already in filter table at index = %d' * 'Invalid ADD MID command: filter table is full' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a command to add a new Message ID to the Packet Filter Table. * The cause of the failure may be an invalid command packet length or an invalid Message ID. * The failure may also result from not having a Packet Filter Table loaded at the time the command was invoked. The loaded table must have an unused entry available for the new Message ID and must not already contain the new Message ID. * The event text will indicate the cause of the failure. |

Table Event ID 67 (Error) - Close All Destination Files

|  |  |
| --- | --- |
| Event ID Number | 67 |
| Event Name | 'Close All Destination Files command (error)' |
| Event Message | 'Invalid DEST CLOSE ALL command length: expected = %d, actual = %d' |
| Type | ERROR |
| Cause | * This event signals the failed execution of a command to close all open Destination Files. The cause of the failure can only be an invalid command packet length. * The event text will indicate the cause of the failure. |

Event Messages - Information

The tables in this section show **information** type event messages for the DS application.

Table Event ID 1 (Informational) - Application Initialization Event

|  |  |
| --- | --- |
| Event ID Number | 1 |
| Event Name | 'Application Initialization Event' |
| Event Message | 'Application initialized, version %d.%d.%d.%d, data at 0x%08X' |
| Type | INFORMATION |
| Cause | This event message is issued when DS has successfully completed its initialization.   * The first %d field contains the Application's Major Version Number. * The second %d field contains the Application's Minor Version Number. * The third %d field contains the Application's Revision Number. * The fourth %d field contains the Application's Mission Revision Number. |

Table Event ID 10 (Informational) - Destination File Table Validation Results

|  |  |
| --- | --- |
| Event ID Number | 10 |
| Event Name | 'Destination File Table Validation Results' |
| Event Message | 'Destination file table verify results: desc text = %s, good = %d, bad = %d, unused = %d' |
| Type | INFORMATION |
| Cause | * This event describes the results of the Destination File Table validation function. The cFE Table Services Manager will call this function autonomously when the default table is loaded at startup and also whenever a table validate command (that targets this table) is processed. * The event text will indicate the descriptor text verification result (OK or bad), the number of table entries that were verified without error (good), the number of table entries that had one or more errors (bad) and the number of unused table entries (unused). Note that the totals also include the results of the verification test for the table description text. Thus, the sum of good + bad + unused results will equal the number of table entries plus one. |

Table Event ID 12 (Informational) – Packet Filter Table Validation Results

|  |  |
| --- | --- |
| Event ID Number | 12 |
| Event Name | 'Packet Filter Table Validation Results' |
| Event Message | 'Filter table verify results: desc text = %s, good = %d, bad = %d, unused = %d' |
| Type | INFORMATION |
| Cause | * This event describes the results of the Packet Filter Table validation function. The cFE Table Services Manager will call this function autonomously when the default table is loaded at startup and also whenever a table validate command (that targets this table) is processed. * The event text will indicate the descriptor text verification result (OK or bad), the number of table entries that were verified without error (good), the number of table entries that had one or more errors (bad) and the number of unused table entries (unused). Note that the totals also include the results of the verification test for the table description text. Thus, the sum of good + bad + unused results will equal the number of table entries plus one. |

Table Event ID 31 (Informational) - No-op

|  |  |
| --- | --- |
| Event ID Number | 31 |
| Event Name | 'No-op command (info)' |
| Event Message | 'NOOP command, Version %d.%d.%d.%d' |
| Type | INFORMATION |
| Cause | * This event signals the successful execution of an application NOOP command. The command is used primarily as an indicator that the DS application can receive commands and generate telemetry. * The first %d field contains the Major Version Number * The second %d field contains the Minor Version Number * The third %d field contains the Revision Number * The fourth %d field contains the Mission Revision Number. |

Event Messages - Debug

The tables in this section show **debug** event messages for the DS application.

Table Event ID 7 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 7 |
| Event Name | 'Table Restored From CDS' |
| Event Message | 'Destination File Table data restored from CDS'  'Filter Table data restored from CDS' |
| Type | DEBUG |
| Cause | * If configured to make DS tables critical, the DS application will try and recover the table data in use prior to a processor reset. * These startup initialization events indicate that the table data has been restored from the CDS. |

Table Event ID 33 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 33 |
| Event Name | 'Reset Housekeeping Counters command' |
| Event Message | 'Reset counters command' |
| Type | DEBUG |
| Cause | This event signals the successful execution of a RESET housekeeping counters command. The command is used primarily to clear counters that have already been examined. |

Table Event ID 35 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 35 |
| Event Name | 'Set Application Enable/Disable State command' |
| Event Message | 'APP STATE command: state = %d' |
| Type | DEBUG |
| Cause | * This event signals the successful execution of a command to set the application enable/disable state for processing data storage packets. The DS application is always enabled to receive and process commands. * The event text will indicate the new setting for the application enable/disable state. |

Table Event ID 37 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 37 |
| Event Name | 'Set Filter File Index command' |
| Event Message | 'FILTER FILE command: MID = 0x%X, index = %d, filter = %d, file = %d' |
| Type | DEBUG |
| Cause | * The Packet Filter Table consists of an array of packet structures, with each element in the array representing one packet Message ID. * Each packet structure contains an array of filter structures, and each filter structure contains a destination file selection. Thus, each packet has multiple filters and each filter selects a file. * File selections are expressed as an index into the Destination File Table. * This event signals the successful execution of a command to set the destination file index for a single filter entry in the Packet Filter Table. * The event text will indicate the packet Message ID, the Packet Filter Table index, the filter array index and the new Destination File Table index selection. |

Table Event ID 39 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 39 |
| Event Name | 'Set Filter Type command' |
| Event Message | 'FILTER TYPE command: MID = 0x%04X, index = %d, filter = %d, type = %d' |
| Type | DEBUG |
| Cause | * The Packet Filter Table consists of an array of packet structures, with each element in the array representing one packet Message ID. * Each packet structure contains an array of filter structures, and each filter structure contains a filter type selection. Thus, each packet has multiple filters and each filter selects a filter type. * This event signals the successful execution of a command to set the filter type for a single filter entry in the Packet Filter Table. * The event text will indicate the packet Message ID, the Packet Filter Table index, the filter array index and the new filter type selection. |

Table Event ID 41 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 41 |
| Event Name | 'Set Filter Parameters command' |
| Event Message | 'FILTER PARMS command: MID = 0x%04X, index = %d, filter = %d, N = %d, X = %d, O = %d' |
| Type | DEBUG |
| Cause | * The Packet Filter Table consists of an array of packet structures, with each element in the array representing one packet Message ID. * Each packet structure contains an array of filter structures, and each filter structure contains a set of filter parameters. Thus, each packet has multiple filters and each filter has unique filter parameters. * This event signals the successful execution of a command to set the filter parameters for a single filter entry in the Packet Filter Table. * The event text will indicate the packet Message ID, the Packet Filter Table index, the filter array index and the new filter parameters (N,X,O). |

Table Event ID 43 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 43 |
| Event Name | 'Set Filename Type command (debug)' |
| Event Message | 'DEST TYPE command: file table index = %d, filename type = %d' |
| Type | DEBUG |
| Cause | * This event signals the successful execution of a command to set the filename type for a Destination File Table entry. * The event text will indicate the Destination File Table index, and the new filename type. |

Table Event ID 45 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 45 |
| Event Name | 'Set File Enable/Disable State command' |
| Event Message | 'DEST STATE command: file table index = %d, file state = %d' |
| Type | DEBUG |
| Cause | * This event signals the successful execution of a command to set the enable/disable state for a Destination File Table entry. * The event text will indicate the Destination File Table index, and the new file enable/disable state. |

Table Event ID 47 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 47 |
| Event Name | 'Set Filename Path command' |
| Event Message | 'DEST PATH command: file table index = %d, pathname = '%s'' |
| Type | DEBUG |
| Cause | * This event signals the successful execution of a command to set the path portion of the filename for a Destination File Table entry. * The event text will indicate the Destination File Table index, and the new filename path text. |

Table Event ID 49 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 49 |
| Event Name | 'Set File Basename command (debug)' |
| Event Message | 'DEST BASE command: file table index = %d, base filename = '%s'' |
| Type | DEBUG |
| Cause | * This event signals the successful execution of a command to set the basename portion of the filename for a Destination File Table entry. * The event text will indicate the Destination File Table index, and the new file basename text. |

Table Event ID 51 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 51 |
| Event Name | 'Set Filename Extension command' |
| Event Message | 'DEST EXT command: file table index = %d, extension = '%s'' |
| Type | DEBUG |
| Cause | * This event signals the successful execution of a command to set the extension portion of the filename for a Destination File Table entry. * The event text will indicate the Destination File Table index, and the new filename extension text. |

Table Event ID 53 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 53 |
| Event Name | 'Set Max File Size command' |
| Event Message | 'DEST SIZE command: file table index = %d, size limit = %d' |
| Type | DEBUG |
| Cause | * This event signals the successful execution of a command to set the file size limit for a Destination File Table entry. * The event text will indicate the Destination File Table index, and the new file size limit. |

Table Event ID 57 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 57 |
| Event Name | 'Set Sequence Count command (debug)' |
| Event Message | 'DEST COUNT command: file table index = %d, sequence count = %d' |
| Type | DEBUG |
| Cause | * This event signals the successful execution of a command to set the sequence count for a Destination File Table entry. * The event text will indicate the Destination File Table index, and the new sequence count. |

Table Event ID 59 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 59 |
| Event Name | 'Close Destination File command' |
| Event Message | 'DEST CLOSE command: file table index = %d' |
| Type | DEBUG |
| Cause | * This event signals the successful execution of a command to close the selected Destination File. * This command will succeed if the Destination File Table index is valid, regardless of whether there was an open file. |

Table Event ID 62 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 62 |
| Event Name | 'Get File Info command' |
| Event Message | 'GET FILE INFO command' |
| Type | DEBUG |
| Cause | * This event signals the successful execution of a command to get the file info diagnostic packet. * The event text will indicate the expected and actual packet size. |

Table Event ID 64 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 64 |
| Event Name | 'Add Message ID to Packet Filter Table command' |
| Event Message | 'ADD MID command: MID = 0x%04X, index = %d' |
| Type | DEBUG |
| Cause | * This event signals the successful execution of a command to add a new Message ID to the Packet Filter Table. * The Packet Filter Table must be loaded and have an unused entry available for adding the new Message ID. The new Message ID must not be zero and must not already exist in the table. |

Table Event ID 66 (Debug)

|  |  |
| --- | --- |
| Event ID Number | 66 |
| Event Name | 'Close All Destination Files command (debug)' |
| Event Message | 'DEST CLOSE ALL command' |
| Type | DEBUG |
| Cause | * This event signals the successful execution of a command to close all open Destination Files. * This command will succeed regardless of whether there was an open file. |

Document Notes

Mission-Specific Conventions

* This document presents selected *information in this dark orange font* that should be removed when tailoring this document for a mission.
* Command and Telemetry mnemonics are mission-specific. This document as delivered has “suggested” names that may or may not be used by the mission when the MOT creates the ground system database. In particular, the suggested names start with $sc\_$cpu\_DS which indicate a global setting for spacecraft, processor selection, and the DS subsystem. This has meaning if the mission has multiple spacecraft, each with a copy of cFE/CFS apps being executed, and/or multiple processors per spacecraft, each with a copy of cFE/CFS apps being executed. Most missions have neither and they do not prepend a $sc\_$cpu\_ selection to the front of the command name. However it is common for missions to differentiate the spacecraft subsystem commands from instrument commands by prepending a couple of characters (e.g. pw for power system) to all the command and telemetry names for that subsystem.
* The nomenclature of command and telemetry mnemonics is highly mission-specific, so this document does not attempt to include the actual command and telemetry database names in advance. For example, for MMS the telemetry mnemonics are defined in an RDL file for ASIST, and they will not exactly match the mnemonics in this Guide.

Tailoring This Document

This section is for anyone tailoring this Guide for a specific mission.

When tailoring this document for a particular mission:

* *Remove or replace text appearing in this dark orange font, with mission-specific values.*
* Review figures to be sure there are no conflicts with mission configurations. Edit figures with MS Visio or MS PowerPoint if necessary.
* Replace CFS defaults with mission defined values in Appendix A.
* Regenerate the table of contents (TOC); add Appendix page prefixes to TOC as needed. Table of Contents, Figures, and Tables can be updated automatically, but the letter prefix for Appendix pages must be added manually after update. To update all figure and table references in the document, when using the PC version of Word, select all, then choose F9.
* When complete, remove Appendix B.

This Guide is formatted using Microsoft Word styles. When adding new sections to the Guide, assign paragraphs to the styles shown in the table below. Center tables and figures horizontally on the page. Use 15% grayscale in new table headings. For bullets in tables, assign the style shown below to set vertical spacing, then assign bullets using the bullet icons menu.

Table 137 Internal Document Styles

| Type | Style to be Used | Justification |
| --- | --- | --- |
| Chapter titles, subtitles, and subsections. | Heading 1 through 6 | Left |
| First level bullets | “List Bullet 1” style. | Left |
| Second level bullets | “List Bullet 2” style | Left |
| Numbered lists | “Style List Enum 0” | Left |
| Names of code modules | Code | N/A |
| All text not otherwise tagged | “Body Text” | Full justification |
| **Tables & Figures** | | |
| First row of tables | Table Header | Center |
| All other cells of tables | Table Cells | Left |
| Figure captions | Caption Figure | Center |
| Table captions | Caption Table | Center |
| Bullets in table cells | “Style Table Cells Vertical” + bullet | Left |